Specifications X5

4.4i; 3.0i

	Body
	
	4.4i
	3.0i
	
	

	No. of doors/seats
	
	5/5
	5/5
	
	

	Length/width/height (unladen)
	mm
	4,667/1,872/1,707
	4,667/1,872/1,715
	
	

	Wheelbase
	mm
	2,820
	2,820
	
	

	Track, front/rear
	mm
	1,576/1,576
	1,576/1,576
	
	

	Turning circle
	m
	12.1
	12.1
	
	

	Fuel tank capacity/range
	ca. ltr
	92
	92
	
	

	Cooling system icl. heater
	ltr
	12.0
	10.5
	
	

	Engine oil
	ltr
	8.0
	6.5
	
	

	Transmission fluid
	ltr
	Lifetime filling
	Lifetime filling
	
	

	Final drive fluid
	ltr
	Lifetime filling
	Lifetime filling
	
	

	Weight, unladen (EU) 
	kg
	2,170
	2,065 (2,090)
	
	

	Max. load
	kg
	555
	610
	
	

	Max permissible weight
	kg
	2,650
	2,600 (2,625)
	
	

	Max permissible axle load1
	kg
	1,230/1,460
	1,230/1,460
1230

	
	

	Max. trailer load1
	
	
	
	
	

	braked (12%)/unbraked
	kg
	2,300/2,700
	2,300/2,300
	
	

	Max. roof load, trailer nose
	kg
	100/120
	100/120
	
	

	Luggage comp. capacity, VDA
	ltr
	465–1,550
	465–1,550
	
	

	Drag coefficient 
	
	
	
	
	

	Front area
	cx x A
	0.36x2.70
	0.35x2.70
	
	

	Engine
	
	
	
	
	

	Layout/No. of cylinders/valves
	
	V90/8/4
	Inline 6/4
	
	

	Engine management
	
	Motronic M 7.2
	Siemens MS 43
	
	

	Displacement, eff.
	cm3
	4398
	2979
	
	

	Bore/stroke
	mm
	92.0/82.7
	84.0/89.6
	
	

	Compression ratio/fuel grade
	:1
	10.0/ROZ 91–982 
	10.2/ROZ 91–982
	
	

	Max. output
	kW/bhp
	210/286
	170/231
	
	

	At engine speed
	rpm
	5,400
	5,900
	
	

	Max. torque
	Nm
	440
	300
	
	

	At engine speed
	rpm
	3,600
	3,500
	
	

	Electronic
	
	
	
	
	

	Battery/location
	Ah/–
	90/luggage comp.
	70/luggage comp.
	
	

	Alternator
	A/W
	150/2,100
	90/1,260
	
	

	Chassis
	
	
	
	
	

	Front suspension
	
	Tie-bar double joint spring-strut axle; small. Positive steering scrub radius;

	
	
	Compensation of transverse forces, anti-dive

	Rear suspension
	
	Integral axle;

	
	
	Multi-dimensional suspension with anti-squat and anti-dive

	Brakes, front
	
	Disc, vented

	Diameter
	mm
	                           332
	332
	
	

	Brakes, rear
	
	Disc

	Diameter
	mm
	                           324                            324
	 
	
	

	Driving stability system
	
	DSC III (HDC, DBC, SC, ABS ASC-X ADB-X)
	
	
	

	Steering


	
	Rack and pinion, power assisted
	

	Overall ratio
	
	21.1
	
	
	

	Type of transmission
	
	ZF 5 HP 24
	ZF C weit (GM 5)
	
	

	Transmission ratio
	I
	
	3.57
	5.09 (3.24)
	
	

	
	II
	
	2.20
	2.80 (2.22)
	
	

	
	III
	
	1.51
	1.76 (1.60)
	
	

	
	IV
	
	1.00
	1.25 (1.00)
	
	

	
	V
	
	0.80
	1.00 (0.75)
	
	

	
	VI
	
	
	
	
	

	
	R
	
	4.10
	4.71 (3.03)
	
	

	Final drive ratio
	
	3.64
	4.1
	
	

	Tyres
	
	235/65R17 
	235/65R17  
	
	

	
	
	104H AS
	104H AS
	
	

	Wheels 
	
	7.5 J x 17 Alu-Guß
	7.5 J x 17 Alu-Guß
	
	

	Performance
	
	
	
	
	

	Power to weight ratio
	kg/kW
	10.0
	11.7 (11.9)
	
	

	Output per litre
	l/kW
	47.7
	57.1
	
	

	Accelaration
	0
	–
	100 km/h
	s
	7.5
	8.5 (8.8)
	
	

	
	0
	–
	1000 m
	s
	
	29.4 (30.3)
	
	

	In 4th gear
	80
	–
	120 km/h
	s
	
	7.6 (–)
	
	

	Top speed
	km/h
	207 (230)3
	202 (202)
	
	

	Fuel consumption
	
	
	
	
	

	EU-cycle
	ltr/100km
	
	
	
	

	EU, urban
	ltr/100km
	18.8
	17.4 (17.5)
	
	

	EU, extra-urban
	ltr/100km
	11.1
	10.0 (10.3)
	
	

	EU, composite
	ltr/100km
	13.9
	12.7 (12.9)
	
	

	CO2 g/km
	g/km
	335
	305 (310)
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	



 Maybe increased under certain conditions
2 Performance and economy figures are based 

  ROZ 98

