

8. Technical specifications

	
	
	X6 xDrive35i
	X6 xDrive50i
	X6 xDrive30d
	X6 xDrive35d

	
	
	
	
	
	

	Body    
	
	
	
	
	

	No of doors/seats       
	
	5/4
	5/4
	5/4
	5/4

	Length/width/height 
	mm
	4,877/1,983/1,6901)
	4,877/1,983/1,6901)
	4,877/1,983/1,6901)
	4,877/1,983/1,6901)

	Wheelbase
	mm
	2,933
	2,933 
	2,933
	2,933

	Track, front/rear       
	mm
	1,644/1,706
	1,644/1,706
	1,644/1,706
	1,644/1,706

	Turning circle
	m
	12.8
	12.8
	12.8
	12.8

	Tank capacity
	approx l
	85
	85
	85
	85

	Cooling system incl heater 
	l
	10.9
	17.2
	10.4
	10.4

	Engine oil4)
	l
	6.5
	8.0
	7.5
	7.5

	Transmission fluid
	l
	lifetime
	lifetime
	lifetime
	lifetime

	Final drive fluid      
	l
	lifetime
	lifetime
	lifetime
	lifetime

	Weight, unladen to EU (DIN)
kg
	2,145 (2,070)
	2,265 (2,190)
	2,150 (2,075)
	2,185 (2,110)

	Max load
	kg
	600 (650)2)
	650
	600 (650)2)
	600 (650)2)

	Max permissible load
	kg
	2,670 (2,720)2)
	2,840
	2,675 (2,725)2)
	2,710 (2,760)2)

	Max axle load, front/rear     
	kg
	1,280/1,470 
(1,290/ 1,510)2) 
	1,400/1,520
	1,280/1,470 
(1,290/1,510)2)
	1,320/1,480 
(1,330/1,520)2)

	Max trailer load
	
	
	
	
	

	braked (12%)  
	kg
	2,700/750
	3,500/750
	2,700/750
	2,700/750

	Max roofload/max download
	kg
	100/120
	100/140 
	100/120
	100/120

	Luggage comp to DIN 70020
	l
	570–1,450
	570–1,450
	570–1,450
	570–1,450

	Air drag         
	Cd x A
	0.34 x 2.82
	0.36 x 2.82
	0.33 x 2.82
	0.34 x 2.82

	
	
	
	
	
	

	Engine
	
	
	
	
	

	Config/No of cyls/valves 
	
	in-line/6/4
	V/8/4
	in-line /6/4
	in-line /6/4

	Engine management
	
	MSD81
	MSD85
	DDE6.2.6
	DDE6.2.6

	Capacity
	cc
	2,979
	4,395
	2,993
	2,993

	Bore/stroke   
	mm
	84.0/89.6
	89.0/88.3
	84.0/90.0
	84.0/90.0

	Compression ratio
	:1
	10.2
	10.0
	17.0
	17.0

	Fuel grade
	
	RON 95–98
	RON 95–98
	Diesel
	Diesel

	Max output
	kW/bhp
	225/306
	300/407
	173/235
	210/286

	at          
	rpm  
	5,800–6,250
	5,500–6,400
	4,000
	4,400

	Max torque 
	Nm
	400
	600
	520
	580

	at         
	rpm  
	1,300–5,000
	1,750–4,500
	2,000–2,750
	1,750–2,250

	
	
	
	
	
	

	Electrical System
	
	
	
	
	

	Battery/installation 
	Ah/–
	90/luggage comp
	90/luggage comp
	90/luggage comp
	90/luggage comp

	Alternator   
	A/W
	210/2,940
	210/2,940
	170/2,380
	170/2,380

	
	
	
	
	
	

	Chassis 
	
	
	
	
	

	Suspension, front   
	
	   Double track arm axle; small, negative steering roll radius; anti-dive

	Suspension, rear    
	
	   Integral axle; space-effect suspension with anti-squat and anti-dive

	Disc brakes, front
	mm
	  Two-piston 
floating calliper
	Single-pist 
frame calliper
	Single-piston 
floating calliper
	Single-piston 
floating calliper

	Diameter
	
	  365 x 36, vented
	385 x 36, vented  
	348 x 30, vented  
	365 x 36, vented  

	Disc brakes, rear
	
	   Single-piston swing calliper

	Diameter   
	mm
	  345 x 24, vented  
	385 x 24, vented  
	320 x 20, vented  
	345 x 24, vented  

	Driving stability systems
	
	   DCS III (HDC, DBC, ABS, ASC-X, ADB-X, DTC, Trailer Stability Control)

	Steering
	
	  

	Steering transmission, overall
	
	
	

	Type of gearbox
	
	   Six-speed automatic with Steptronic, electronic gear selector lever and shift paddles
   on steering wheel

	Gear ratios
I
	:1
	4.171
	4.171
	4.171
	4.171

	
II
	:1
	2.340
	2.340
	2.340
	2.340

	
III
	:1
	1.521
	1.521
	1.521
	1.521

	
IV
	:1
	1.143
	1.143
	1.143
	1.143

	
V
	:1
	0.867
	0.867
	0.867
	0.867

	
VI
	:1
	0.691
	0.691
	0.691
	0.691

	
R
	:1
	3.403
	3.403
	3.403
	3.403

	Final drive          
	:1
	3.909
	3.636
	3.636
	3.636

	Tyres, front/rear      
	
	255/50 R19 107V XL RSC
	255/50 R19 107W XL RSC
	  255/50 R19 107V XL RSC
	255/50 R19 107V 
XL RSC

	Rims, front/rear
	
	9J x 19 light-alloy
	9J x 19 light-alloy
	9J x 19 light-alloy
	9J x 19 light-alloy


	
	
	X6 xDrive35i
	X6 xDrive50i
	X6 xDrive30d
	X6 xDrive35d

	
	
	
	
	
	

	Performance     
	
	
	
	
	

	Power-to-weight ratio
to DIN 
	kg/kW
	9.2
	7.3
	12.0
	10.0

	Output per litre
	kW/l
	75.5
	68.3
	57.8
	70.2

	Acceleration
0–62mph
	s
	6.7
	5.4
	8.0
	6.9

	
0–1000 m/h
s
s
	27.2
	24.6
	29.1
	27.3

	In 4th/5th gear 50-75mph
s

s
	–/–

	–/–
	–/–
	–/–

	Top speed            
	mph
	149
	155
	130 (137)3)
	147

	
	
	
	
	
	

	Fuel Consumption in EU Cycle
	
	
	
	

	Urban    
	mpg
	19.0
14,9
	16.0
	27.2
	26.9

	Extra-urban   
	mpg
	32.8
	29.7
	40.4
	39.8

	Composite 
	mpg
	25.9
	22.6
	34.4
	34.0

	CO2
	g/km
	262
	299
	217
	220

	
	
	
	
	
	

	Miscellaneous 
	
	
	
	
	

	Emission rating     
	
	EU4 
	EU4 
	EU4 
	EU4

	Embankment angle, front/rear
°
°
	25.1/25.5
	25.1/25.5
	25.1/25.5
	25.1/25.5

	Ramp angle
	°
	19.1
	19.1
	19.1
	19.1

	Ground clearance, unladen
	mm
	212
	212
	212
	212

	Perm. all-wheel drive 
	
	variable
	variable
	variable
	variable


Specifications in ACEA markets/data relevant to homologation in part for Germany only (weight)

1) Height incl roof railing: 1,699 mm 
2) With Adaptive Drive and/or self-levelling with pneumatic suspension

3) With high-speed set-up (market-specific)
4) Oil change amount





































