

7. Technical specifications

	Bodyshell
	
	M3 Saloon  
	
	
	

	No of doors/seats
	 
	4/5
	
	
	

	Length/width/height (EU,unladen)

)
	mm
	4,580/1,817/1,447
	
	
	

	Wheelbase
	mm
	2,761
	
	
	

	Track, front/rear
	mm
	1,540/1,539
	
	
	

	Turning circle
	m
	11.7
	
	
	

	Tank capacity
	approx ltr
	63
	
	
	

	Cooling system incl heater     

l
	ltr
	11.4
	
	
	

	Engine oil
	ltr
	8.8
	
	
	

	Transmission fluid
	ltr
	2.1
	
	
	

	Final drive fluid  
	ltr
	1.2
	
	
	

	Weight, unladen, to DIN1
	kg
	1,605
	
	
	

	Weight, unladen, to  EU2
	kg
	1,680
	
	
	

	Max load to DIN
	kg
	545
	
	
	

	Max permissible weight to DIN
	kg
	2,150
	
	
	

	Max axle load, front/rear    
	kg
	1,020/1,190
	
	
	

	Max trailer load3
	
	–
	
	
	

	braked (12%)/unbraked  
	kg
	–
	
	
	

	Max roof load/max towbar downl.
	kg
	75/– 
	
	
	

	Luggage comp to DIN
	ltr
	450
	
	
	

	Air drag
	cd x 
	0.673
	
	
	

	Power Unit
	
	
	
	
	

	Config/No of cyls/valves     Zylinder/Ventile


	 
	V/8/4
	
	
	

	Engine management
	 
	MS S60
	
	
	

	Capacity 
	cc
	3,999
	
	
	

	Bore/stroke
	mm
	92.0/75.2
	
	
	

	Compression ratio
	: 1
	       12.0 : 1 
	
	
	

	Fuel grade
	RO
	98 (95)
	
	
	

	Max output @ rpm
	kW/hp 
	309/420 @ 8,300
	
	
	

	Max torque @ rpm
	Nm/lb-ft
	400/295 @ 3,900
	
	
	

	Electrical System
	
	
	
	
	

	Battery/installation
	Ah/–
	70/luggage compartment
	
	
	

	Alternator
	A/W
	180/2,520
	
	
	

	Chassis and Suspension
	
	
	
	
	

	Suspension, front   
	 
	   Aluminium two-joint spring strut axle with tiebar; 

	
	
	   small positive steering roll radius; compensation of transverse forces; anti-dive

	Suspension, rear   
	
	   Five-arm axle with   

	
	
	   anti-squat and anti-dive   

	Brakes, front
	
	   Single-piston swing-calliper compound disc brakes

	Diameter   
	mm
	   360 x 30, vented and cross-drilled
	
	
	

	Brakes, rear  
	 
	   Single-piston swing-calliper compound disc brakes

	Diameter    
	mm
	   350 x 24, vented and cross-drilled
	
	
	

	Driving stability systems
	 
	   ABS, ASC, CBC, DSC; Variable M Differential Lock 

	Steering
	 
	   Rack-and-pinion with hydraulic assistance and Servotronic

	Steering transmission, overall
	: 1 
	12.5
	
	

	Gearbox, type
	
	ZFG
	
	
	

	Gear ratios
I 
	: 1 
	4.055
	
	
	

	
II
	: 1 
	2.396
	
	
	

	
III
	: 1 
	1.582
	
	
	

	
IV
	: 1 
	1.192
	
	
	

	
V
	: 1 
	1.000
	
	
	

	
VI
	: 1 
	0.872
	
	
	

	
VII
	: 1
	–
	
	
	

	
R
	: 1 
	3.678
	
	
	

	Final drive           
	: 1 
	3.846
	
	
	

	Tyres, front/rear
	 
	245/40 ZR18/265/40 ZR18 
	

	Rims, front/rear
	 
	   8.5 J x 18 EH2 + IS 29 cast aluminium/9.5 J x 18 EH2 + IS 23 cast aluminium

	Performance   
	
	
	
	
	

	Power-to-weight ratio, DIN
	kg/kW
	5.2
	
	
	

	Power-to-weight ratio, DIN
	kg/hp
	3.8
	
	
	

	Output per litre
	kW/ltr
	77.3
	
	
	

	Output per litre
	hp/ltr
	105.0
	
	
	

	Acceleration 0–62mph
	sec
	4.9
	
	
	

	Top speed           
	mph
	1554
	
	
	

	Fuel Consumption in EU Cycle
	
	
	
	
	

	Urban    
	mpg
	15.8
	
	
	

	Extra-urban   
	mpg
	30.7
	
	
	

	Composite 
	mpg
	22.8
	
	
	

	CO2 
	g/k
	295
	
	
	

	Miscellaneous
	
	
	
	
	

	Emission standard   
	
	EU4
	
	
	



Weight of vehicle in road trim (DIN).


2Weight of vehicle in road trim (DIN) plus 75 kg for driver and luggage.

3May be increased under certain conditions.              

4Electronically limited. 





































