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•
Concept innovation: as the creator of the Sports Activity Vehicle, 
BMW is now presenting the world’s first Sports Activity Coupé.

•
The BMW X6 offers a brand-new, innovative interpretation of the features and design qualities typical of a large BMW Coupé. And at the same time 
it is the most sporting and dynamic rendition of a BMW X Model. 
Through its design alone, the BMW X6 authentically visualises superior driving dynamics and outstanding supremacy. 

•
Individual and extravagant looks: sporting, striking front end with large 
air intakes, stretched side-line, low greenhouse, clear emphasis 
on the wheels as an expression of powerful presence, classic coupé proportions, generous, convex-concave surfaces, sweeping flow 
of the roofline into the powerful rear end.

•
The BMW X6 comes as standard with BMW’s intelligent xDrive 
all-wheel drive technology and is the first vehicle in the world to offer 
Dynamic Performance Control for unique agility, tracking stability, precision and traction in every situation. Variable distribution of drive power is 
thus ensured not just between the front and rear axle – by xDrive – but 
also, by means of Dynamic Performance Control, between the two 
rear wheels, left and right. This maintains a superior stabilising function even under sudden load change and in overrun.

•
Newly developed top-of-the-range power unit: V8 petrol engine with 
Twin Turbo technology and direct petrol injection (High Precision Injection), the world’s first 8-cylinder petrol engine with the turbo-charger and 
catalytic converters housed in the V-section between the two rows of cylinders. This innovative arrangement ensures uniquely compact dimensions and serves to reduce pressure losses on the intake and 
exhaust side. Capacity 4,395 cc, max output 300 kW/407 hp from 
5,500–6,400 rpm, max torque 600 Nm/442 lb-ft from 1,750–4,500 rpm. Most efficient engine in its class, outperforming ULEV II and EU5 
emission standards, BMW EfficientDynamics combined with maximum power and performance.

•
Unique range of power units: V8 petrol engine with Twin Turbo 
(300 kW/407 bhp), in-line 6-cylinder with Twin Turbo (225 kW/306 bhp), 
in-line 6-cylinder diesel with Variable Twin Turbo (210 kW/286 bhp), 
in-line 6-cylinder diesel with turbocharger (173 kW/235 bhp). 

•
Six-speed automatic transmission with optimised gearshift dynamics standard on all engine variants, extremely fast gearshift, supreme 
shift comfort, optimisation of fuel economy by converter lock-up clutch operating largely free of slip, electronic gear selector lever 
and gearshift paddles on the steering wheel featured as standard. 

•
The BMW X6 boasts a body structure conceived and designed for maximum occupant safety. In combination with the car’s passive safety systems, this fulfils all prerequisites for excellent results in all crash-tests relevant the world over. Occupant safety is ensured among other things 
by three-point inertia-reel seat belts on all seats, frontal and side airbags 
as well as head airbags at the side, and crash-activated headrests at 
the front. Bi-xenon dual headlights including a daytime light function, fog lamps, two-stage brake lights, and runflat tyres all come as standard.

•
Innovative body and interior concept: 4-door coupé with large tailgate opening far up to the top, high-quality, sophisticated interior with 
a sporty and luxurious ambience, four seats, large, highly adjustable luggage compartment (570–1,450 litres/20.0–50.8 cu ft).

•
Interior design underlining the outstanding, sporting character of the 
BMW X6. Leather sports steering wheel with multifunction buttons and gearshift paddles featured as standard, centre console with knee pads 
for the driver and front passenger, front seats with versatile adjustment, in part electric, two rear seats with individual seat contours typical 
of a coupé and integrated headrests. 

•
Suspension and driver assistance systems (optional) exclusive to BMW: Adaptive Drive (anti-roll and adaptive dampers), Active Steering, Head-Up Display, Adaptive Headlights with variable light distribution and turning 
light, High Beam Assistant, cruise control with brake function.

•
Wide range of comfort functions and innovative entertainment options: BMW iDrive with personalised favourite buttons, CD-player compatible 
with an MP3, AUX-in bush featured as standard, USP socket, multichannel audio system, DVD system at the rear, 4-zone automatic air conditioning, Active Seat Ventilation, back-up camera, navigation systems, BMW Assist, BMW Online, BMW TeleServices optional. 

•
The BMW X6 is manufactured exclusively for the world market at the 
BMW Spartanburg plant in South Carolina/USA according to the company’s high quality standards which apply worldwide. Production at this site 
is highly flexible according to customer wishes. Currently, the BMW X6, BMW X5 and BMW Z4 are built on a shared assembly line at the Spartanburg plant.

•
Engine variants:
BMW X6 xDrive50i: V8 petrol engine with Twin Turbo 
and direct injection (High Precision Injection) 
Capacity 4,395 cc, max output 300 kW/407 bhp from 5,500–6,400 rpm, max. torque from 600 Nm/442 lb-ft from 1,750–4,500 rpm, 
Acceleration [0–100 km/h] in 5.4 seconds,
Top speed 250 km/h (155 mph),
Average fuel consumption to EU standard 12.5 litres/100 km 
(22.6 mpg imp),
CO2 emissions to EU standard 299 g/km.

BMW X6 xDrive35i: in-line 6-cylinder petrol engine with Twin Turbo and
direct injection (High Precision Injection)
Capacity 2,979 cc, max output 225 kW/306 bhp from 5,800–6,250 rpm,
max. torque 400 Nm/295 lb-ft from 1,300–5,000 rpm,
Acceleration [0–100 km/h] in 6.7 seconds,
Top speed 240 km/h (149 mph),
Average fuel consumption to EU standard 10.9 litres/100 km 
(25.9 mpg imp),
CO2 emissions to EU standard 262 g/km.


BMW X6 xDrive35d: in-line 6-cylinder diesel engine with Variable Twin Turbo and third-generation common rail fuel injection
Capacity 2,993 cc, max output 210 kW/286 bhp at 4,400 rpm,
max torque 580 Nm /427 lb-ft at 1,750–2,250 rpm,
Acceleration [0–100 km/h] in 6.9 seconds,
Top speed 236 km/h (146 mph),
Average fuel consumption to EU standard 8.3 litres/100 km (34.0 mpg imp),
CO2 emissions to EU standard 220 g/km.



BMW X6 xDrive30d: in-line 6-cylinder diesel with turbocharger and
third-generation common-rail direct fuel injection
Capacity 2,993 cc, max. output 173 kW/235 bhp at 4,000 rpm,
max. torque 520 Nm/383 lb-ft from 2,000–2,750 rpm,
Acceleration [0–100 km/h] in 8.0 seconds
Top speed 210 km/h (130 mph), 220 km/h (136 mph) with optional high speed adaptation
Average fuel consumption to EU standard 8.2 litres/100 km
(34.4 mpg imp),
CO2 emissions to EU standard 217 g/km.
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