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Technical specifications.
BMW i3 50 xDrive as First Edition.
	
	
	BMW i3 50 xDrive as First Edition

	
	
	

	Vehicle Category
	
	

	Drive type / body style
	
	Battery-electric vehicle (BEV) / Sports Activity Vehicle (SAV)

	
	
	

	Body
	
	

	No. of doors / seats
	
	4 / 5

	Length/width/height (unladen)
	mm
	4760 / 1865 / 1480

	Wheelbase
	mm
	2897

	Track, front/rear
	mm
	1606 / 1613

	Turning circle
	m
	12.2

	Weight, unladen (DIN/EU)
	kg
	2205 / 2280

	Max. load to DIN
	kg
	505

	Max. permissible weight
	kg
	2710

	Max. axle load, front/rear
	kg
	1260 / 1490

	Max. trailer load,
braked (12%)/unbraked
	
kg
	
1800 / 750

	Max. roofload/towbar download
	kg
	75 / 75

	Luggage comp. capacity
	l
	420 

	Additional storage comp. under bonnet
	l
	31

	Air resistance
	cX x A
	0.21 x 2.35

	
	
	

	Power Unit
	
	

	Drive concept
	 
	Electric all-wheel drive, coordinated transmission of the drive torque from two electric motors to the front and rear wheels respectively, as required

	Max. output
	kW/hp
	345 / 469

	Max. torque
	Nm
	645

	Power-to-weight ratio
	kg/kW
	6.4

	Type of transmission
	
	Automatic transmission, single-speed 

	
	
	

	Electric motors
	
	

	Motor technology
	 
	Sixth-generation BMW eDrive technology: 
electrically excited synchronous motor at the rear axle, asynchronous motor at the front axle, each sharing a housing with the power electronics and transmission; generator function for recuperating energy

	Front Electric Motor
	
	

	Motor designation
	
	HF1002N0

	Peak output to ECE R 85
	kW/hp
	123 / 167

	at
	rpm
	4607

	Max. torque
	Nm
	255

	at
	rpm
	0 – 4607

	Gear ratio
	:1
	8.801

	Rear Electric Motor
	
	

	Motor designation
	
	HD1001N0

	Peak output to ECE R 85
	kW/hp
	240 / 326

	at
	rpm
	5500

	Max. torque
	Nm
	435

	at
	rpm
	0 – 5000

	Gear ratio
	:1
	9.606

	
	
	

	High-voltage Battery
	
	

	Storage technology
	
	Lithium-ion

	Installation
	
	Underfloor

	Voltage
	V
	698.9

	Energy capacity, net
	kWh
	108.7

	Charging time, 0 – 100 % charge
	
	11h at 11 kW (16 A / 230 V, three-phase AC, wallbox)

	Charging time, 0 – 100 % charge
	
	5h 30m at 22 kW (32 A / 230 V, three-phase AC, wallbox)

	Charging time, 10 – 80 % charge
	
	21 min at 400 kW (800 V, DC, fast-charging station)

	Additional range after 10 minutes of 
DC charging (max. charging rate) 1)
	
km
	
320 – 423

	
	
	

	Charging
	
	

	Max. charging rate 
AC, three-phase
	
kW
	
11.0 (optional: 22.0)

	Max. charging rate 
DC
	
kW
	
400

	
	
	




	
	
	BMW i3 50 xDrive as First Edition

	
	
	

	Bidirectional Charging
	
	

	Vehicle-to-Load (optional), 
max. rate (AC)
	kW
	3.7

	Vehicle-to-Home, max. rate (DC)
	kW
	11.0

	Vehicle-to-Grid, max. rate (DC)
	kW
	11.0

	
	
	

	Driving Dynamics and Safety
	
	

	Suspension, front
	
	Double-joint spring strut axle in lightweight aluminium-steel construction with torque arm and anti-roll bar. Trapezoidal shear panels forming connection between axle subframe, high-voltage battery and body

	Suspension, rear
	
	Five-link axle in lightweight aluminium-steel construction with separately arranged springs and dampers

	Brakes, front
	
	Vented disc brakes, with single-piston floating callipers

	Brake disc size
	mm
	370

	Brakes, rear
	
	Vented disc brakes, with single-piston floating callipers

	Brake disc size
	mm
	370

	Driving stability systems
	
	Standard: Heart of Joy integrated drivetrain and driving dynamics management, integrated braking system, DSC incl. ABS, ASC and DTC (Dynamic Traction Control), CBC (Cornering Brake Control), Dry Braking function, Fading Compensation, Start-Off Assistant, HDC (Hill Descent Control), trailer stability control

	Safety equipment
	
	Standard: airbags for driver and front passenger, side airbags for driver and front passenger, interaction airbag between driver and front passenger, head airbags for front and rear seats, three-point inertia-reel seatbelts on all seats with belt tensioner and belt force limiter in the front, crash sensors, tyre pressure indicator

	Steering
	
	Electric Power Steering (EPS) 
with Servotronic function

	Steering wheel turns (lock to lock)
	
	2.7

	Tyres, front/rear
	
	255/45 R 19 102 W/Y XL

	Rims, front/rear
	
	8J x 19 light-alloy

	
	
	

	Performance
	
	

	Acceleration	0–100 km/h
	s
	4.7

	Top speed
	km/h
	200 

	
	
	

	Consumption / Range (WLTP combined)
	
	

	Electric power consumption
as per EnVKV
	
kWh/100 km
	
16.1 – 13.5

	Attainable electric power cons. 
in individual configuration
	
kWh/100 km
	
16.1 – 13.5

	Electric power consumption 
motorway 2)
	
kWh/100 km
	
19.7 – 16.8

	Range as per EnVKV
	km
	758 – 906

	Attainable range in individual configuration
	
km
	
758 – 906

	
	
	

	Environmental Characteristics
	
	

	Pass-by noise
	dB(A)
	66

	Emission rating
	
	Electric vehicle

	CO2 class(es) as per EnVKV
	
	A



Specifications apply to ACEA markets/data relevant to homologation applies in part only to Germany
All of the stated equipment features, technical data and fuel/electric power consumption and emissions figures relate to the offering in the German market. The figures refer to a vehicle with basic configuration in Germany. These may vary depending on the wheel/tyre size and items of optional equipment selected.

Official electric power consumption and range figures were determined based on the prescribed WLTP measurement procedure and are in accordance with the Pkw-EnVKV. Further information can be found at www.bmw.de

1) The extra range added after ten minutes of high-power charging was calculated in accordance with ISO 12906 based on the WLTP cycle. Both this and charging performance are dependent on vehicle equipment, the battery’s charge level and age, battery temperature, the individual driving profile, use of auxiliary consumers, the ambient temperature and the charging station’s available charging power.
2) Corresponds to WLTP Extra High


Exterior and interior dimensions.
BMW i3 50 xDrive as First Edition.








The dimensions indicated in the technical drawing are in millimetres and may vary depending on the model and items of optional equipment fitted.
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