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9.  Specifications
	Body

d

Anzahl Türen / s
	
	M6

	
	

	No. of doors/seats
	
	2/2 + 2
	
	

	Length/width/height (unladen) 
	mm
	4,871/1,855/1,377
	
	

	Wheelbase
	mm
	2,781
	
	

	Track, front/rear
	mm
	1,567/1,584
	
	

	Turning circle
	m
	12.5
	
	

	Fuel tank capacity/range
	approx. ltr
	70
	
	

	Cooling system incl. heater
	ltr
	15.0
	
	

	Engine oil
	ltr
	13.0
	
	

	Transmission fluid
	ltr
	1.2
	
	

	Final drive fluid
	ltr
	                                  2.6
	
	

	Weight, unladen (EU)1
	kg
	1,710
	
	

	Max. load (DIN)
	kg
	                             415
	
	

	Max. permissible weight (DIN)
	kg
	2,200
	
	

	Max. permissible axle load front/rear
	kg
	1,090/1,200
	
	

	Max. trailer load2
	
	
	
	

	braked (12%)/unbraked
	kg
	–
	
	

	Max. roof load/trailer nose weight
	kg
	–
	
	

	Luggage comp. capacity, VDA
	ltr
	450
	
	

	Drag coefficient
	cX x A
	0.32 x 2.15
	
	

	Engine
	
	
	
	

	Layout/No. of cylinders/valves
	
	V 90/10/4
	
	

	Engine management
	
	MS S65
	
	

	Displacement
	cc
	4,999
	
	

	Bore/stroke
	mm
	92.0/75.2
	
	

	Compression
	:1
	12.0 
	
	

	Fuel grade3
	RON
	95–98
	
	

	Max. output
	kW/bhp
	373/507
	
	

	At engine speed
	rpm
	7,750
	
	

	Max. torque
	Nm
	520
	
	

	At engine speed
	rpm
	6,100
	
	

	Electronic
	
	
	
	

	Battery/location
	Ah/–
	90/Boot
	
	

	Alternator
	A/W
	1,70/2,380
	
	

	Chassis
	
	
	
	

	Front suspension
	
	Double-joint thrust-rod spring strut axle in aluminium; 
compensation of transverse forces; anti-dive.

	Rear suspension
	
	Integral axle (aluminium), wheel suspension with special effect 
anti-squat/anti-dive

	Brakes, front
	
	Single-piston floating-caliper disc brakes

	Diameter
	mm
	348, vented
	
	

	Brakes, rear
	
	Single-piston floating-caliper disc brakes

	Diameter
	mm
	                345, vented
	
	

	Driving stability system
	
	ABS, DSC, CBC 

	Steering
	
	Rack-and-pinion, power-assisted

	Overall ratio
	:1
	                            12,4
	
	

	Type of transmission
	
	SMGlll
	
	

	Transmission ratio     
	I
	3.985
	3.985
	

	
	II
	2.652
	2.652
	
	

	
	III
	1.806
	1.806
	
	

	
	IV
	1.392
	1.392
	
	

	
	V
	1.159
	1.159
	
	

	
	VI
	1
	1
	
	

	
	Vll
	0.833
	0.833
	
	

	
	R
	3.985
	3.985
	
	

	Final drive ratio
	:1
	3.62
	
	 

	Tyres, front
	
	255/40 ZR19
	
	

	Tyres, rear
	
	285/35 ZR19
	
	

	Wheels, front
	
	8,5J x 19 EH 2 IS 12 Alu
	
	

	Wheels, rear 
	
	9,5J x 19 EH 2 IS 28 Alu
	
	 

	Performance
	
	
	
	

	Power to weight ratio (DIN)
	kg/kW
	4.6
	
	

	Output per litre
	ltr/kW
	74.6
	
	

	Acceleration
  0–100 km/h
	s
	4.6
	
	

	In 4th/5th gear
80–120 km/h
	
	4.4/5.8
	
	

	Top speed
	Km/h
	                           2502
	
	

	Fuel consumption (EU cycle)
	
	
	
	

	urban
	ltr/100 km
	22.7
	
	

	extra-urban
	ltr/100 km
	10.2
	
	

	composite
	ltr/100 km
	14.8
	
	

	CO2 
	g/km
	357
	
	

	Miscellaneous
	
	
	
	

	Emission classification
	
	
	
	


The values given in parenthesis apply to the automatic transmission.

1Weight of the car in road trim (DIN) plus 75 kg for driver and luggage. 

2Deviations are possible under certain conditions.

3Performance and consumption figures relate to RON 98.





































