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1.
The BMW X6.
Description in Brief. 
 2

2.
World Debut of the First Sports Activity Coupé:
The BMW X6 (short version). 
 5

•
Concept innovation: As the creator of the Sports Activity Vehicle, BMW is now presenting the world’s first Sports Activity Coupé.

•
The BMW X6 offers a brand-new, innovative interpretation of the features and design qualities typical of a large BMW Coupé. And at the same time 
it is the most sporting and dynamic rendition of a BMW X Model. Through 
its design alone, the BMW X6 authentically visualises superior driving dynamics and outstanding supremacy. 

•
Individual and extravagant looks: Sporting, striking front end with large air intakes, stretched side-line, low greenhouse, clear emphasis on the 
wheels as an expression of powerful presence, classic coupé proportions, generous, convex-concave surfaces, sweeping flow of the roofline into 
the powerful rear end.

•
The BMW X6 comes as standard with BMW’s intelligent xDrive all-wheel drive technology and is the first vehicle in the world to offer Dynamic 
Performance Control for unique agility, tracking stability, precision and traction in every situation. Variable distribution of drive power is thus ensured not just between the front and rear axle – by xDrive – but also, through Dynamic Performance Control, between the two rear wheels 
left and right. This maintains a superior stabilising function even under sudden load change and in overrun.

•
Newly developed top-of-the-range power unit: V8 gasoline engine with Twin Turbo technology and direct gasoline injection (High Precision Injection), the world’s first eight-cylinder gasoline engine with the turbo-charger and catalytic converters housed in the V-section between the 
two rows of cylinders. This innovative arrangement ensures uniquely compact dimensions and serves to reduce pressure losses on the intake and exhaust side. Capacity 4,395 cc, max output 300 kW from 5,500–6,400 rpm, max torque 600 Nm from 1,750–4,500 rpm. Most efficient engine in its class, outperforming ULEV II and EU5 emission standards, BMW EfficientDynamics combined with maximum power 
and performance. 

•
Unique range of power units: V8 gasoline engine with Twin Turbo (300 kW), straight-six with Twin Turbo (225 kWhp), straight-six diesel with Variable Twin Turbo (200 kW). 

•
Six-speed automatic transmission with optimised gearshift dynamics standard on all engine variants, extremely fast gearshift, supreme 
shift comfort, optimisation of fuel economy by converter lock-up clutch operating largely free of slip, electronic gear selector lever and gearshift paddles on the steering wheel featured as standard. 

•
The BMW X6 boasts a body structure conceived and designed for maximum occupant safety. In combination with the car’s passive 
safety systems, this fulfils all prerequisites for excellent results in all crash-tests relevant the world over. Occupant safety is ensured inter alia by 
three-point inertia-reel seat belts on all seats, frontal and side airbags as well as head airbags at the side, and crash-activated headrests at the 
front. Bi-xenon dual headlights including a daytime light function, foglamps, 
two-stage brake lights, and runflat tyres all come as standard.

•
Innovative body and interior concept: Four-door coupé with large tailgate opening far up to the top, high-quality, sophisticated interior with a sporty and luxurious ambience, four seats, large, highly adjustable luggage compartment (570–1,450 litres).

•
Interior design underlining the outstanding, sporting character of the 
BMW X6. Leather sports steering wheel with multifunction buttons and gearshift paddles featured as standard, centre console with kneepads 
for the driver and front passenger, front seats with versatile adjustment, 
in part electric, two rear seats with individual seat contours typical 
of a coupé and integrated headrests. 

•
Suspension and driver assistance systems (optional) exclusive to BMW: Adaptive Drive (anti-roll and adaptive dampers), Active Steering, Head-Up Display, Adaptive Headlights, Bending Lights, High-Beam Assistant, 
cruise control with brake function.

•
Wide range of comfort functions and innovative entertainment options: BMW iDrive with personalised favourite buttons, CD-player compatible with an MP3, AUX-in bush featured as standard, USP socket, multi-channel audio system, DVD system at the rear, four-zone automatic air conditioning, active seat ventilation, back-up camera and navigation systems optional. 

•
Engine variants:
BMW X6 xDrive35i: Straight-six gasoline engine with Twin Turbo and 
direct injection (High Precision Injection) 
Capacity 2,979 cc, max output 225 kW from 5,800–6,250 rpm,  
  max torque 400 Nm from 1,300–5,000 rpm, 
Acceleration [0–100 km/h] in 6.7 seconds,
Top speed 240 km/h, 
Average fuel consumption to EU standard 10.9 litres/100 km 
CO2 emissions to EU standard 262 g/ km, 
Available in South Africa 07/2008.

BMW X6 xDrive35d: Straight-six diesel engine with Variable Twin Turbo and third-generation common rail fuel injection 
Capacity 2,993 cc, max output 210 kW at 4,400 rpm, 
max torque 580 Nm at 1,750–2,250 rpm,
Acceleration [0–100 km/h] in 6.9 seconds, 
Top speed 236 km/h, 
Average fuel consumption to EU standard 8.3 litres/100 km, 
CO2 emissions to EU standard 220 g/ km, 
Available in South Africa 07/2008.

BMW X6 xDrive50i: V8 gasoline engine with Twin Turbo and 
direct injection (High Precision Injection) 
Capacity 4,395 cc, max output 300 kW from 5,500–6,400 rpm, 
max torque from 600 Nm from 1,750–4,500 rpm, 
Acceleration [0–100 km/h] in 5.4 seconds, 
Top speed 250 km/h, 
Average fuel consumption to EU standard 12.5 litres/100 km, 
CO2 emissions to EU standard 299 g/km, 
Available in South Africa 01/2009.


The world’s first Sports Activity Coupé, the BMW X6 – shown as a concept car for the first time at the IAA in Frankfurt earlier this year – is ready for the road and will go on sale in South Africa in the middle of 2008. 

With an unpre​cedented combination of on-road dynamic performance, so typical of the BMW brand, and the unique supremacy typical of all BMW X models on all tracks and terrain, the BMW X6 enters the market with the commitment to introduce a radical change in mentality.

With its low side window areas and a roofline dropping smoothly to the rear, the BMW X6 clearly offers all the proportions of a genuine, fully-fledged coupé. Inside, the new model – again in typical coupé style – provides ample space for the driver and front passengers as well as two further occupants 
at the rear, travelling on generously dimensioned rear seats in sporting design, with individual seat contours and integrated headrests. 

Yet, at the same time, enhanced ground clearance, flared wheel arches in striking design, four doors, a large rear lid as well as the high waistline all bear out a clear styling resem​blance to the other models in the BMW X range. This design is indeed an authentic expression of the dynamic driving potential offered by the BMW X6 through its drivetrain and suspension technology not only on the road, but also on rough terrain.
And it’s that drivetrain and suspension technology that will allow the BMW X6 to establish a new benchmark in all-wheel drive driving dynamics and prowess when the first two of three X6 models is launched in the middle of 2008.
Featuring BMW’s intelligent xDrive all-wheel-drive technology with electronic control for variable distribution of drive power between the front and rear axles, the chassis and drivetrain of the BMW X6 consistently adjusts to driving conditions at all times and in all situations. At the same time, BMW’s ICM Integrated Chassis Management high-performance electronic control ensures perfect harmony of drivetrain and suspension functions within fractions of a second, spelling out maximum stability and supreme performance wherever you go and at all times. 
A world-first: 

Dynamic Performance Control for superior agility.

Standard on the BMW X6, and featured for the first time on any BMW model in the world, Dynamic Performance Control ensures variable distribution of drive forces between the two rear wheels. A world-first, this cutting-edge technology significantly enhances steering precision and, as a result, the agility of the vehicle from low speeds whenever required. In fast bends with abrupt steering manoeuvres or when the driver suddenly decelerates, Dynamic Performance Control serves to further improve the stability of the entire vehicle, allowing the driver to safely enjoy new dimensions of driving dynamics. On slippery or uneven surfaces, finally, Dynamic Performance Control provides the further advantage of even safer and more stable traction.
Superior dynamics with Twin Turbo engines across the range.

This superior drivetrain and suspension technology, allows the BMW X6 to convert all the power of the engine safely and consistently into driving dynamics under virtually all conditions and on all kinds of surfaces. And the power units available in the first Sports Activity Coupé set standards themselves in terms of muscular performance, superior running smoothness, and outstanding efficiency in their respective class. 
The top-of-the-range BMW X6 xDrive50i (only available in South Africa in early 2009) is powered by an all-new eight-cylinder, while the BMW X6 xDrive35i (available at launch in mid-2008) features the most powerful straight-six within the BMW engine portfolio. Significantly, both of these gasoline engines benefit in their performance characteristics and efficiency from the exclusive combination of Twin Turbo technology and High Precision Injection available only from BMW. The principle of combining two turbochargers and direct gasoline injection applied for the first time on the straight-six is now also to be admired on the new V8. 

The BMW X6 xDrive35d (available at launch in mid-2008) is entering the market with the world’s most sporting and dynamic six-cylinder diesel with Variable Twin Turbo technology and 210kW of power. 
A class of its own: 
The new eight-cylinder with Twin Turbo Technology.

Supremacy is the feature that applies to all of BMW’s X Models and to all of BMW’s eight-cylinder power units. And now the BMW X6 is adding 
an incomparably dynamic variant to the line-up of BMW X Models, with 
the world’s first Sports Activity Coupé for the first time boasting a particularly sporting and dynamic eight-cylinder.
Displacing 4.4 litres, the new V8 power unit in the BMW X6 xDrive50i features Twin Turbo technology and direct gasoline injection (High Precision Injection) allowing a maximum output of 300 kW throughout a broad range of engine speed from 5,500–6,400 rpm. Engine torque reaches its peak of 600 Newton-metres throughout an unusually large speed range from 1,750–4,500 rpm. The spontaneous, intense and long-lasting thrust generated in this way is the result of Twin Turbo technology already featured on BMW’s most powerful straight-six combined with High Precision Injection. 
On the new V8 the cooling effect of direct fuel injection also ensures a compression ratio quite unusual on a turbocharged power unit, helping to 
give the engine an even higher level of all-round efficiency.

The position of the turbochargers and catalytic converters in the V-section between the two rows of cylinders is likewise an innovation in technology allowing particularly compact engine dimensions and at the same time requiring new configuration of the intake and exhaust ducts. This means shorter intake and exhaust manifolds and larger cross-sections significantly reducing pressure losses on both the intake and exhaust side.

The all-aluminium V8 power unit developed for the BMW X6 offers all the qualities typical of an eight-cylinder in incomparably sporting style. In practice this means a combination of superior torque at low engine speeds with an ongoing surge of power and performance up to the higher speed range. 

The BMW X6 xDrive50i accelerates from 0–100 km/h in just 5.4 seconds and boasts ample power reserves for fascinating acceleration also at higher speeds. Top speed is a truly impressive 250 km/h limited electronically by the engine control unit. 

The new V8 power unit is also the most efficient engine in its class. Combined with a number of further technologies developed in the overall context of BMW EfficientDynamics, the engine gives the BMW X6 xDrive50i fuel consumption and emission figures significantly better than other eight-cylinder vehicles competing with the BMW X Models. Average fuel consumption of the BMW X6 xDrive50i is 12.5 litres/100 km, while the CO2 rating is 299 grams per kilometre.
The BMW X6 xDrive50i will only be available in South Africa in 2009.
BMW’s most powerful straight-six in the world’s first 
Sports Activity Coupé.

The second gasoline-powered version of the BMW X6 boasts the most powerful straight-six within BMW’s engine portfolio and will be available at the launch of the new BMW X6 in South Africa in the middle of next year. Maximum output of the engine featured in the BMW X6 xDrive35i is 225 kW from an engine capacity of 3.0 litres. 
This superior power is maintained consistently between 5,800 and 6,250 rpm by the 2007 World Engine of the Year, with maximum torque of 400 Newton-metres provided all the way from 1,300–5,000 rpm. This gives the six-cylinder superior power and performance from an unusually early point on a gasoline engine, subsequently maintaining this high power throughout a broad range of engine speed.
Like the new V8 power unit, the engine in the BMW X6 xDrive35i offers the exclusive combination of Twin Turbo technology and High Precision Injection available only from BMW for incomparable power and performance plus a standard of economy quite unique in comparison with the engine’s dynamic driving potential.

The BMW X6 xDrive35i accelerates from 0–100 km/h in just 6.7 seconds and boasts a top speed of 240 km/h. At the same time, fuel consumption is a modest 10.9 litres per 100km on the combined EU cycle. 

Maximum diesel power: straight-six with Variable Twin Turbo.

Two turbochargers, direct fuel injection, optimum performance – the most powerful BMW diesel engine ever available in South Africa will show a number of interesting features quite comparable to the two gasoline engines when it is launched in the BMW X6 in the middle of 2008. 
Indeed, the 3.0-litre straight-six diesel with Variable Twin Turbo (VTT) technology is a truly outstanding engine in every respect, developing 210 kW at 4,400 rpm as the most sporting power unit of its kind the world over. At the same time the BMW X6 xDrive35d boasts its own, unique characteristics and a wide range of equally unique technical features.
This outstanding power unit impressively underlines BMW’s great competence also in the development of the diesel engine. With its all-aluminium crankcase, VTT turbocharging and third-generation common-rail fuel injection featuring piezo-injectors, the engine offers ideal qualities for impressive power and performance combined with outstanding efficiency. 

Weighing just 194 kg, this high-performance diesel is some 50 kilos lighter than an eight-cylinder with roughly the same output – an advantage again benefiting the dynamic driving character of the BMW X6 xDrive35d. 

Thanks to this superior power, acceleration to 100 km/h comes in 6.9 seconds and the top speed of the BMW X6 xDrive35d is 236 km/h. Compared with this kind of performance, average fuel consumption in the EU test cycle of just 8.3 litres/100 kilometres is even more impressive. 

BMW EfficientDynamics: wide range of features serving to reduce fuel consumption and emissions – and all coming as standard.

Offering a wide range of features serving to enhance efficiency on and 
around the engine, all versions of the new BMW X6 ensure a particularly good balance of power, performance and economy – and all these features come 
as standard.
Brake Energy Regeneration on all engine variants, to mention just one example, ensures intelligent management of the flow of energy concentrating the generation of electricity for the on-board network on the overrun and brake application phases. This serves to consistently charge the battery, without extracting power from the engine and, as a result, without using any of the energy provided by the fuel. As long as the engine is pulling the car, on the other hand, the alternator generally remains disconnected and not in use. 

Apart from outstanding efficiency in the generation of electric power, this also serves to provide more power for acceleration and thus for enjoying an even more dynamic style of motoring.

The all-round efficiency of the BMW X6 is further optimised by on-demand control and activation of the engine’s ancillary units helping, inter alia, to significantly reduce the power required for the fuel and steering assistance pumps and thus again saving energy in the process.

The drive belt for the a/c compressor, to present another example, comes 
with an independent clutch automatically disconnecting the compressor as soon as the driver switches off the air conditioning and thus reducing the 
drag forces generated by the compressor to a minimum. 

Automatic transmission designed for sports motoring.

Power is transmitted on the BMW X6 in standard trim by a six-speed automatic transmission with a particularly sporting gearshift now enhanced to an even higher level. 
The automatic transmission chooses the appropriate gear with incomparable spontaneity, precision and efficiency, benefiting not only the superior comfort, but also the supreme driving dynamics of the BMW X6. Being directly connected to the engine, incorporating a converter clutch operating largely without slip, and allowing particularly precise choice of gears, the six-speed automatic transmission also helps to optimise the overall efficiency of 
the power unit in practice. 

The automatic transmission shifts gears either in response to the electronic gear selector lever or the gearshift paddles on the steering wheel. The shift pattern on the gear selector lever is the same as on a conventional automatic transmission, but with the selector level returning to its starting point after each gearshift.

Transmission management is not mechanical, but rather goes through electrical signals. To activate the manual gear selection mode, all the driver has to do is press the selector lever to the left. Then he is able to shift gears in sequence by hand – either from the gear selector lever or through the gearshift paddles featured as standard on the steering wheel: Pulling one of the paddles out serves to shift up gears, pressing the paddle serves to shift down.

Using this paddle gearshift, the driver is able to shift gears with maximum spontaneity in a manual mode. So whenever he operates one of the paddles, the transmission will shift immediately also from the automatic mode into manual gearshift.
Pricing announced in 2008.

Further technical details of the new BMW X6, along with pricing, will be announced in the  second quarter of 2008.

###

If you have any questions, please contact:

BMW South Africa Corporate Communications

Guy Kilfoil, Manager: Automotive Communications

Telephone: +27 12 522 2227, fax: +27 11 805 2775

Media website: www.quickpic.co.za

e-mail: guy.kilfoil@bmw.co.za 












The BMW X6.�Contents.

















2.	World Debut of the First�Sports Activity Coupé:�The BMW X6.





1.	The BMW X6.�Description in Brief.








