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•
World premiere: the first Sports Activity Coupé.

•
BMW underpins its innovative strength in the segment 
of the X models.

•
Unique driving dynamics – authentically visualised in design.
The BMW X6 is unmistakably a member of the BMW X family. It has a 
large number of the qualities which also distinguish the Sports Activity Vehicle 
BMW X5. But at the same time it reinterprets the character of the BMW 
X models: with a clear focus on driving dynamics, also expressed in its design. The BMW X6 combines the supremacy, seating position and versatility 
of a Sports Activity Vehicle with the elegance and sporty driving qualities of a large BMW coupé. The result of this combination is an entirely new vehicle category: the Sports Activity Coupé.

With the invention of the Sports Activity Vehicle (SAV), BMW already founded 
a vehicle category which was both innovative and pioneering. The BMW X5 launched in 1999 instantly took up a leading position within the competitive environment due to its fascinatingly dynamic character. With the new BMW X5, this superior driving dynamics became even more marked in what has since become a hotly competed segment. The success of the BMW X5 is clear evidence of the fact that sporty driving properties have an important role 
to play in this segment too. The BMW X6 thus represents the logical further development of the range of BMW X models. Its innovative vehicle concept realises the dynamic performance which is characteristic of BMW in 
a way which is even more specifically targeted. 

Innovative drivetrain technology, unique design: the BMW X6.

The aim in developing the BMW X6 was to enable a driving experience determined by sporty flair which would be unequalled to date within 
the competitive environment of the X models. At the same time, this core quality was to be visualised in a fascinating and equally unique design. 
For this reason, the world’s first Sports Activity Vehicle is equipped with innovations in the field of drivetrain and chassis technology which allow the driving dynamics of a BMW X model to reach a whole new dimension. Particularly important here are Dynamic Performance – unique the world 
over – and the new 8-cylinder engine with Twin Turbo and High Precision Injection, presented in the BMW X6 for the first time.

The newly developed V8 power unit is at the top of the engine range for then BMW X6. For the first time BMW combines Twin Turbo supercharging and direct petrol injection in an 8-cylinder engine. The 300 kW/407 bhp power unit is also the world’s first V8 petrol engine in which the turbocharger is located between the cylinder banks. An unusual feature for an 8-cylinder, apart from the compact layout, is its degree of economy. The V8 with Twin Turbo and 
High Precision Injection by BMW is the most efficient engine in its category

Greater agility, precision and ride stability thanks to 
Dynamic Performance Control.

In addition to the intelligent all-wheel drive system BMW xDrive, Dynamic Performance Control also offers a further increase in agility, steering precision, traction on bends, ride stability and supremacy off the road. It is presented 
in the BMW X6 for the first time and comes as standard. While xDrive ensures 
a continuously variable and adaptable distribution of drive torque between 
the front and rear axle, Dynamic Performance Control likewise takes care of variable distribution of the drive forces between the two real wheels. The system operates independently of propulsion power and ensures the stability of the vehicle even if the driver makes abrupt steering manoeuvres or suddenly releases the accelerator. Dynamic Performance Control thus provides a secure advance into a new dimension of driving dynamics. 

The standard fittings of the BMW X6 also include other special features which enhance the sporty driving experience provided by this vehicle. Shift paddles at the steering wheel enable fast and reliable handling of the 6-speed automatic transmission in manual shift mode. Knee pads at the central console provide additional stability for the driver and front passenger on avoidance manoeuvres or on unsecured surfaces. Two single seats at the rear with integrated headrests also ensure that rear passengers enjoy sound lateral support on 
fast bends.

Authentic, impressive and distinctive: the design.

The outstanding driving properties of the BMW X6 are reflected in a distinctive design. The world’s first Sports Activity Coupé gives a visual impression of 
its dynamic potential at first sight. What is more, its appearance is ideally suited to demonstrating individual style. 

The lines of the BMW X6 are clearly those of a big BMW coupé. It is defined 
by the sweeping transition of the elegantly stretched roof line into the powerful rear section. Enhanced ground clearance, strikingly flared wheel arches, four doors and a large tailgate as well as the high waistline bear out a clear styling resemblance to the other BMW X models. In this combination, the design reveals a consistent focus on sportiness and elegant present, giving a clear indication of the driving properties of the BMW X6. In the same way, 
the BMW X6 with its impressive dynamic performance confirms all the expectations aroused by its unique design.

Innovative strength in a growing market segment.

By presenting the BMW X6, BMW once more demonstrates its outstanding expertise in the development of new vehicle concepts. The world’s first Sports Activity Coupé interprets the brand’s characteristic sporty flair in an entirely new way. What is more, the family of BMW X models gains a new and extremely fascinating member. The world’s first Sports Activity Coupé once again shows BMW to be a driving force within a market segment characterised by especially dynamic growth. What is more, both with its concept and its drivetrain technology, the BMW X6 shows the outstanding innovative strength of the world’s most successful manufacturer of premium vehicles.


•
Proportions of a coupé and characteristic features of a 
BMW X model – combined in one vehicle for the first time.

•
Innovative design reflects outstanding driving dynamics.

•
Luxurious sporty flair inside the vehicle.

The BMW X6 sets out to change habitual perspectives. It enriches the idea 
of a BMW coupé by adding a new, attractive facet and thus enables a 
whole new perspective on the family of BMW X models. With its flat side window surfaces and a roof line which falls gently to the rear, the BMW X6 clearly has the proportions of a coupé. On the inside – equally typical of 
a coupé – it offers space for the driver, front passenger and two additional passengers. The latter travel on generously sized single rear seats with a sporty design and integrated headrests. The raised ground clearance, strikingly 
flared wheel arches, four doors and a large tailgate bear out a clear styling resemblance to the other BMW x models. This design is an authentic expression of the dynamic potential provided by the drivetrain and chassis technology of the BMW X6, not just on the road but also off the beaten track. 

Unique design: dynamic lines, powerful presence.

The design of the BMW X6 reveals a vehicle which clearly has BMW X genes, though it interprets the character of this type of model in a uniquely sporty fashion. The design is the authentic visualisation of outstanding driving properties which in the BMW X6 are largely defined by the intelligent all-wheel drive system BMW xDrive, including Dynamic Performance Control and the extended track width. 

The BMW X6 is definitely a genuine BMW from every angle. This is ensured first and foremost by the sculptural design so characteristic of all 
BMW X models. The front section, the sides and the rear section flow smoothly 
and directly into one another, the various forms and surfaces merging to provide one harmonious entity. Various design features typical of the brand also come out clearly in the car’s details, ranging from the BMW kidney grille, 
the dual round headlights optically “cut off” at the top and the powerful contour line along the side and including the horizontal lines at the rear emphasising 
the sheer width of the vehicle.

Front end with dynamic orientation to the road.

In the new Sports Activity Coupé, even the impression of the front end ensures a powerful presence. Due to the greater share of surfaces finished in body colour, however, the front end looks lower, thereby emphasising the dynamic orientation of the BMW X6 to the road. The BMW X genes are also revealed in the engine compartment lid and the structure of the vertically positioned 
BMW kidney grille with its rods finished in a sophisticated titanium colour in 
the BMW X6 xDrive50i and the BMW X6 xDrive35d, and in black in the 
other model variants. 

Large air intake flaps positioned far to the outside bear clear testimony not 
only to the cooling requirements of the powerful engines. Interacting with the 
side paddles extending far to the inside over the headlights, the air scoops 
also provide clear orientation towards the wheels, emphasising the powerful 
stance of the vehicle of the road. The side air intakes are split horizontally 
by aluminium-coloured bars also bearing the surrounds on the round 
fog lamps. The central air intake in the bumper is wider towards the base, 
so its contours also enhance the visual orientation towards the road.

Through their clearly cut profile at the top, the dual round headlights so 
typical of BMW offer a particularly intense and clearly focussed look. 
The concentrated focus of the entire vehicle on the road appears even stronger and more dramatic. The headlights themselves merge in a dynamic sweeping line into the side panels, the surface of the engine compartment lid is 
divided by striking lines tapering out towards the BMW kidney grille like the borderlines of the engine compartment lid at the sides. The side panels extending far over the headlights towards the middle of the vehicle and powerfully contoured to the outside, finally, highlight the supreme presence 
of the BMW X6 from the front.

Side view: dynamic roofline, muscular surfaces.

The unique proportions of the new BMW X6 come out particularly clearly 
from the side. The short body overhang at the front emphasises the dynamic look of the vehicle, the roof line tapering out gently towards the rear and 
the long body overhang on the rear section adding to the stretched silhouette of a genuine coupé. The roofline reaches its highest point directly above the first row of seats, thus clearly placing the focus on the driver, creating a special effect most appropriate to the extravagant design of the BMW X6. At the 
rear the side window frame features the “counter-swing” at the bottom of the 
D-pillar – so well-known as the “Hofmeister kick”. Chrome surrounds on 
the windows featured as standard distinguish the BMW X6 xDrive50i from 
the other model variants.

The high waistline and powerfully contoured wheel arches both front and 
rear, moving the visual centre of gravity to the middle of the vehicle and 
thus bearing testimony to all-wheel drive, are further significant features of 
the DNA of a BMW X Model. Slender plastic protectors at the bottom 
of the bumpers, side sills and wheel arches also serve to discreetly highlight 
the robust character of the BMW X6.

The side panel is split by two lines with striking contours, moving slowly towards one another at the front end of the vehicle to create a wedge-like impression symbolising the forward-pushing, powerful character of the 
BMW X6. The contour line running parallel to the door openers offers 
a particularly muscular look, enhancing the dynamic wedge shape generated by the growing distance between the shoulder line and the side-sill line 
towards the rear of the vehicle. Extending all the way to the rear light clusters, the contour line visually stretches the entire vehicle to provide an even 
more dynamic and powerful impression. The second character line runs parallel to the side sills half-way between the contour and the side sill lines. At both front and rear, this additional character line ends where the extra-large wheel arches curve powerfully out of the side panels.

While the lines at the side highlight the supreme elegance of the car, 
the special design of the surface gives the BMW X6 a particularly powerful 
look from this perspective. Striking interaction of the concave and convex surfaces emphasises the muscular look of the vehicle, the BMW X6 thus providing an excellent balance between visual power and stylish presence. 

Rear end characterised by strong shoulders and a powerful stance 
on the road.
Features and characteristics typical of elegance, sportiness and robustness likewise come together in fascinating style at the rear end to form a harmonious entity. A powerful bumper and the protector panel on the underfloor are classical elements of a BMW X model in its design. At the same time the new vehicle comes in the proportions typical of a coupé but in the special style 
and class of a BMW X model. The greenhouse with its unusually angled 
rear window tapers out smoothly to the rear, the rear hatch with its striking airflow spoiler adding a further feature typical of a coupé.

The entire rear view is split up by horizontal lines giving the rear end of the BMW X6 an even wider look and emphasising the powerful stance of the car on the road. The rear section achieves its full width in the area of the wheel arches. And the two exhaust tailpipes, positioned far to the outside and 


set in high-quality trim, draw the onlooker’s attention to the wheels. The striking light edge in the lower section of the bumper creates a further accentuation, highlighting the ground clearance of the BMW X6 which is characteristic of the BMW X models.

Even the rear lights, in their design, highlight the unique character of the 
BMW X6, re-interpreting the L-shape so typical of a BMW X model and adding a dynamic, sweeping look. The rear lights reach far into the side panels, ensuring that the entire breadth of the vehicle comes into its own in its night-time design.

Sporty and exclusive interior.

Down to the very last detail, the interior of the BMW X6 offers a unique synthesis of exclusive luxury, sporting dynamics, and powerful style. Tense surfaces swivelling into one another symbolise the active character of 
BMW’s Sports Activity Coupé, sporting features such as knee pads on both sides of the centre console, paddles on the sports steering wheel featured 
as standard, and the fine scale on the circular instruments creating an excitingly different driving experience in the new BMW X6 both on the road and off 
the beaten track.

Like all BMW x models, the new Sports Activity Coupé offers the occupants on all four seats an elevated, commanding seating position. In particular, this 
gives the driver a clear feeling of being perfectly in control of his BMW X6 in all situations. In conjunction with the cockpit simply begging the driver to drive 
his vehicle in active style, this creates an innovative impression of genuine, 
all-out sportiness. The driver’s and front passenger’s seats come as standard with electric seat and backrest angle adjustment. A further point distinguishing the world’s first Sports Activity Coupé from the other BMW X models is the sporting design of the individual rear seats separated from one another through the centre console, the high-rising side supports and the integrated headrests.

The BMW X6 is the only car in the complete entire segment of the 
BMW X models to feature a sports steering wheel with gearshift paddles 
as standard. These paddles enable the driver to shift gears manually on 
the six-speed automatic transmission. Multifunction buttons on the steering wheel serve furthermore to operate the telephone and audio systems 
quickly, smoothly and without the slightest distraction. The high-quality trim on the steering wheel comes as standard in leather and features a highlight 
bar finished in pearl gloss chrome.

The instrument panel is dominated by dual circular instruments with fine 
scales reminiscent of motor racing as a clear visual reference to the sporting character of the BMW X6. The galvanised trim rings on the instrument 
panel clearly accentuate the exclusive character of the vehicle’s interior, with the same high-quality metal shimmer on the rotary knobs, the door 
openers, on the gearshift lever knob and the brackets within the air vents.

The new knee pads on the centre console stand out clearly as a particularly sporting feature offering the driver and front passenger additional stability 
in avoidance manoeuvres in city traffic and when driving off-road over uneven surfaces. The high-quality knee pad supports made of glass fibre-reinforced plastic combine low weight with outstanding robustness. Depending on 
the features and equipment within the vehicle, the knee pads are matched 
to the colour of the respective interior and finished in various materials.

Excellent quality of finish and a wide range of storage options.
Visibly and tangibly sophisticated, high-class surfaces make the interior 
of the BMW X6 a genuine experience to touch and see at all times. Through their special quality designed for lasting strength and resistance, the interior surfaces also emphasise the idea of robustness. The special surface grain 
on the instrument panel is formed by innovative IM (in-mould) coating. Optional leather finish on the instrument panel ensures a particularly exclusive effect 
in its touch and looks brought out by the use of high-quality leather and seams as well as smooth and gentle padding beneath the leather surface.

In its design, the dashboard is reminiscent of a firm but resistant band swivelling from one side to the other. This dynamic design then continues within the door linings with their twin-section trimming, the glove compartment merging elegantly and unobtrusively into the surrounding surfaces. Locking automatically together with the doors, the glove compartment does not 
require a separate lock, the two-piece lid opening upwards and downwards to provide convenient access to the fully illuminated storage space inside.

The spacious storage box in the centre console opens and closes in the 
same way by means of a so-called butterfly lid. Further features on the 
centre console are the two extra-large cupholders complete with a lid on top serving also to hold even bottles firmly in position. Two further large cupholders are provided in the rear console, together with an additional storage box. 
And spacious storage pockets in the door panels front and rear, finally, round 
off the wide range of storage facilities.

Lots of space, lots of customisation options.

Wide opening rear doors facilitate access to the two rear seats, and 
headroom also at the rear is unusually generous for a coupé: a seat height 
of 944 millimetres or 37.2" guarantees supreme comfort and convenience 
even for tall passengers. Seen from the rear, the window graphics in the 
BMW X6 generate a feeling of forward-pushing openness and, as a result a generous sensation of spaciousness and abundance.

A wide range of materials and colours highlighting the sporting character of 
the BMW X6 adds to the individual style and personality of this unique vehicle. The exterior paintwork, for example, comes in a choice of no less than ten colours, while five equipment variants, two interior colours and five trim options provides a wide range of possible combinations. Trim bars in ash grain and flywheel aluminium have been created especially for BMW’s Sports Activity Coupé. And while the wood variant exudes a particular touch of discreet exclusivity, the sweeping polish on the aluminium version shows a clear and distinct reference to motor racing. Looking at the seat covers, the customer has the choice of various high-quality cloth and leather variants as well as a new combination of alcantara/leather developed exclusively for the BMW X6. In this version, the alcantara cover in the middle of the seats is combined with 
fine-grain Oregon leather at the sides.

The Lights Package is yet another option, LED units around the door handles and light bars in the door pockets providing a stylish and sophisticated ambience inside the car and facilitating use of the control elements housed 
in the door panels. A further important point is that the Lights Package 
also illuminates the area outside the car and comes with exit lights in the 
door linings.

•
World premiere: Dynamic Performance Control.

•
Dynamic performance with intelligent control: 
Integrated Chassis Management.

•
Even greater supremacy with Active Steering and Adaptive Drive.

A new type of vehicle and a new driving experience: the BMW X6 
definitely offers the best of both worlds. In terms of driving dynamics, the world’s first-ever Sports Activity Coupé offers new dimensions defined 
by a considerable enhancement of agility, unique stability on fast bends and 
safe traction on slippery surfaces. Powerful engines, BMW’s intelligent xDrive all-wheel drive technology, DSC (Dynamic Stability Control), optional 
Active Steering and Adaptive Drive as well as Dynamic Performance Control featured for the first time in the BMW X6 as a standard feature: together 
with the extended track width of the rear axle, these set the foundation for superior driving dynamics.

Even with a moderate, reserved style of motoring, Dynamic Performance Control optimises steering precision very noticeably, enabling the BMW X6 to handle even difficult driving conditions and demonstrate the outstanding quality of its drive and suspension technology. 

Driving dynamics with intelligent control: 
Integrated Chassis Management. 

The vehicle’s drivetrain and suspension systems interact perfectly 
with BMW’s ICM Integrated Chassis Management. This high-performance electronic control ensures perfect harmony of drivetrain and suspension functions within fractions of a second, spelling out maximum stability and supreme performance wherever you go and at all times. Even when a sudden change in driving conditions occurs, for example on varying surfaces, during spontaneous steering manoeuvres or when accelerating or applying the brake abruptly, ICM reacts with utmost precision to the xDrive, DSC and Dynamic Performance Control actuators and to Active Steering when fitted as an option. In all cases, the nature and scope of such intervention is appropriately masterminded to ensure not just maximum driving stability, but also optimum dynamics.

BMW’s X models already available today owe their outstanding agility largely 
to the supreme performance and qualities of ICM. Now the central control 
unit has an even more progressive influence on driving dynamics in the new 
BMW X6, since it is also able to use the actuators serving BMW’s new Dynamic Performance Control: depending on driving conditions and with 
fully variable management, the power of the engine is no longer split “just” between the front and rear axle, but also – due to Dynamic Performance Control – between the left and right rear wheel, feeding additional power to the 
most appropriate point where it can be conveyed best to the road. This drive technology – which is quite unique in the market – enhances the agility, steering precision and tracking stability of the car in bends as well as its traction on slippery surfaces, significantly improving driving dynamics. As a result, Dynamic Stability Control is only required to intervene by means of selective brake application to the appropriate wheel or wheels when the vehicle really reaches the extreme physical limits. The world’s first Sports Activity Coupé thus offers the driver the truly fascinating experience of being able to 
handle even the most demanding driving situations with a level of sporting 
style and dynamic performance never seen before. 

The drivetrain and suspension technology of the BMW X6 ensures the highest conceivable level of safety, precision and driving pleasure on all surfaces. 
The foundation for this is provided by suspension technology which is quite unique in the segment of the BMW X models. The front axle is a double 
track control arm configuration applying the double joint principle for dynamic lateral acceleration, superior tracking stability and minimisation of forces 
acting on the steering wheel. Appropriate front axle kinematics ensure optimum front wheel camber on the road at all times, so the BMW X6 maintains supreme grip and road-holding even under the most dynamic conditions. 

At the rear the BMW X6 features BMW’s patented Integral IV axle serving 
to harmonise superior comfort with equally superior dynamics. And now 
this lightweight construction has been specifically optimised for the 
Sports Activity Coupé in numerous details, the entire rear axle configuration being appropriately adjusted to the specific demands made of this model 
for supreme sportiness and performance. The wheel mounts, rear axle subframe and four track arms efficiently take up the dynamic and drive forces flowing into the suspension, reducing any elastic distortion of the wheel mounts, while soft swinging mounts provide appropriate longitudinal suspension and optimise the roll quality of the wheels. Effectively separating the road surface from the drivetrain, the rear axle helps to ensure first-class noise control and ride comfort.

The BMW X6 comes as standard on 19-inch light-alloy wheels. Also featured as standard, runflat safety tyres enable the driver to continue even after a complete loss of pressure in the tyres smoothly and safely to the nearest workshop. Yet another feature is the Tyre Damage Indicator which permanently monitors air pressure and warns the driver as soon as the pressure of air 
in the tyres drops more than 30 per cent below the ideal level by means of an visual signal in the instrument cluster. 

BMW xDrive: intelligent al-wheel drive for enhanced dynamics 
and optimum traction.

Permanent all-wheel drive with electronically controlled, variable distribution 
of drive power between the front and rear axles gives all BMW X models 
not only superior traction, but also enhanced driving dynamics. Indeed, 
BMW xDrive gains its superiority as an intelligent all-wheel-drive system by feeding drive power through a distributor box with an electronically controlled multiple-plate clutch according to driving conditions in exactly the right dosage to the appropriate axle with optimum grip on the road. The possibilities for optimising drive power and thrust in this way, in the interests of both driving stability and dynamic performance, are further enhanced by the use of 
Dynamic Performance Control in the BMW X6, now also varying the distri-
bution of power between the right and left-hand rear wheel.

In normal driving situations BMW xDrive distributes drive power in a 40 : 60 split front-to-rear, with sensors consistently measuring wheel slip. Hence the system is able within fraction of a second to vary the distribution of drive forces, with BMW xDrive – unlike conventional all-wheel drive systems – anticipating the upcoming situation and not just responding once a wheel has started to spin. This serves to stabilise the vehicle even before the driver notices any need for action.

Offering advantages of this calibre, BMW xDrive enhances the dynamic performance of the BMW X6 by counteracting even the slightest tendency to over steer or understeer right from the start at the earliest conceivable point. And now, incorporating BMW’s new Dynamic Performance Control, xDrive is able to respond even more quickly and in line with current requirements, the positive effects on driving dynamics being particularly significant on fast bends. 

Unparalleled agility and tracking stability thanks to xDrive and 
Dynamic Performance Control.

The positive effect of Dynamic Performance Control on the agility of the 
BMW X6 comes out clearly even in conventional everyday traffic, the vehicle steering into bends with significantly enhanced precision even when 
travelling at moderate speeds. Unlike a conventional locking differential, Dynamic performance Control cause the outside wheel to accelerate, 
for example. The additional momentum thus generated is realised as a yaw 
or steering movement of the vehicle. Additional supremacy is provided 
by Dynamic Performance Control for sudden steering manoeuvres and at particularly high speeds on bends.
With a vehicle possibly pushing to the outside of a bend when driving to 
the limit either at the rear or on its front wheels, depending on road 
conditions, the angle of the bend and road speed, both BMW xDrive and Dynamic Performance Control are able to counteract both of these manifestations of driving instability: as soon as the vehicle threatens 
to oversteer, xDrive reduces the transmission of power to the rear wheels pushing to the outside. And now Dynamic Performance Control also 
comes in, withdrawing drive forces from the outer rear wheel in a bend subject to particular centrifugal loads and diverting these forces to the inner rear 
wheel, thus creating an outward yaw moment. This intervention in the interest of greater stability is so quick and finely controlled that the driver will 
not even notice what is happening. What he will notice, however, is that 
the BMW X6 ensures exceptional steering precision even when 
driving dynamically.

Operating exactly the other way round, Dynamic Performance Control also counteracts any tendency to understeer: xDrive reduces the transmission 
of power to the front wheels “pushing” to the outside, Dynamic Performance Control shifts drive power to the outer rear wheel on a bend in the interests 
of optimum stability and an inward yaw moment. As a result, the car steers even more smoothly and precisely into the bend, following the course set by the driver with greater agility and enhanced tracking stability, regardless 
of road speed.
Unique: Dynamic Performance Control increases steering precision, even when the driver takes his foot off the accelerator.

A further particular feature of Dynamic Performance Control is that engine power and torque are split variably between the rear wheels not only when the engine is “pulling” the vehicle, but also in overrun. This is ensured by an additional, superimposed transmission unit within the final drive made up of a double planetary gearset and a multiple-plate clutch operated by an electric motor, varying the distribution of drive power even when the driver takes 
his foot off the accelerator. The BMW X6 is the first vehicle in the world to offer such a stabilising effect independent of engine load and drive power.

Dynamic Performance Control also serves to optimise traction on a slippery surface: the ability to vary the transmission of engine power specifically as required – now also between the two rear wheels – serves among other things to improve traction and puling force whenever the vehicle is running on different surfaces from one side to the other, for example with asphalt on one side and a snowbound surface on the other. Any differences in the frictional coefficient between the wheels on the left and right (modal split) are set 
of by Dynamic Performance Control specifically sharing out drive forces on 
the rear axle.

By taking just one look at the instrument cluster, the driver receives a clear message showing activity of Dynamic Performance Control and xDrive: 
a graphic display presented as an alternative to the other displays on the 
on-board computer simply accessed by pressing the lever on the steering 
column informs the driver of the current distribution of drive power. 
In a symbolic graphic presentation of the four drive wheels, bar diagrams 
show how much power is going to each wheel at any given point in time. 

DSC only intervenes in the threshold range.

The difference in drive forces between the two rear wheels provided by Dynamic Performance Control may go all the way to 1,800 Newton-metres. But even then, all the driver will feel when Dynamic Performance Control intervenes is an increase in agility, traction and driving stability – albeit 
a significant one. Another effect he will also feel and appreciate thanks to Dynamic Performance Control is that DSC Dynamic Stability Control intervenes much less frequently than before. In practice, this means that the driver is 
able to use the full drive power and torque of the engine much longer than with a conventional system, DSC acting on individual wheels or reducing engine power only when the driver really pushes the car to the physical threshold of performance.

Over and above this stabilising effect, DSC in the new BMW X6 offers a wide range of additional functions serving to promote safe and dynamic motoring. These include ABS, Automatic Stability Control (ASC), Trailer Stability Control, Hill Descent Control (HDC), Dynamic Brake Control (DBD) automatically maximising brake pressure when required in the interest of minimum stopping distances, Cornering Brake Control (CBC) and finally standard cruise control with its own brake application function. The Automatic Differential Brake 
(ADB) serves as a transverse lock between the two wheels, with the fading compensation function increasing brake pressure as required under extremely high brake temperatures. Meanwhile regular dry braking optimises brake performance in wet conditions while the Start-Off Assistant enables the driver to set off more smoothly and easily on an uphill gradient. The BMW X6 features a parking brake operating both electromechanically and hydraulically and activated or released simply by pushing a button. The parking brake 
is fitted with an Auto Hold function which especially increases comfort in 
stop-and-go traffic.

Reflecting the high standard of driving dynamics provided by the BMW X6, DSC also comes with Dynamic Traction Control (DTC) as a special function, raising the DSC response thresholds to a higher level and allowing a 
particularly sporting and active style of motoring, and enabling the driver to 
set off smoothly on snow or loose sand with the drive wheels intentionally spinning slightly.

Supported by a wide range of DSC functions, the high-performance brake system featured in the BMW X6 ensures excellent stopping power in all conditions. Inner-vented discs on all four wheels take up brake energy, newly developed lightweight brakes featuring 385 millimetre discs and aluminium floating callipers front and rear guarantee extremely good resistance to fading and maximum brake comfort in the top-of-the-range BMW X6 xDrive50i. 
The lightweight brake discs are riveted onto an aluminium cover, following 
a principle patented by BMW and now also emulated by other vehicle manufacturers in order to significantly reduce unsprung masses and prevent deformation of the discs on account of high temperatures even under extremely high brake loads. 

Active Steering for a sporty and comfortable style of motoring.

The rack-and-pinion steering in the BMW X6 varies the steering transmission ratio as a function of the steering angle, thus meeting all kinds of requirements under different driving conditions. Keeping power assistance at a consistent level also at high speeds with the steering in its midrange position, the steering thus enhances superior control of the car. On bends the driver benefits from 
a more direct steering response, the steering ratio being geared to the angle of the steering wheel and thus allowing an even more dynamic style of motoring.

As an option, the BMW X6 is also available with Active Steering. This very special system developed by BMW offers exactly the right steering ratio at 
all speeds, maintaining direct steering behaviour up to a speed of about 
90 km/h or 55 mph, as required particularly for a sporting and active style of motoring. A further advantage in this case is that the driver only has to turn 
the steering wheel twice from lock to lock when parking. At higher speeds, on 
the other hand, Active Steering offers a more indirect transmission ratio in 
the interests of steady directional stability and, as a result, enhanced motoring comfort.

In the BMW X6, Active Steering is combined with Servotronic, thus increasing steering comfort due to reduced forces depending on road speed. What 
is more, Active Steering makes an active contribution in stabilising the car in the event of oversteer on bends or for particularly demanding brake manoeuvres. When applying the brakes on surfaces which differ from left to right, for example – the so-called modal split brake manoeuvre – Active Steering countersteers discreetly but firmly to prevent the car from swerving out of control. 

Unique: Adaptive Drive with data transfer via FlexRay.
Carefully harmonised interaction of the vehicle’s anti-roll bars and dampers masterminded by Adaptive Drive is another unique feature in the segment 
of BMW X models. Indeed, this combination of active body roll control 
and variable damper adjustment also available as an option gives the new BMW X6 incomparably superior driving response.

By means of sensors in the vehicle, Adaptive Drive permanently monitors 
and calculates data on road speed, steering angle, longitudinal and 
lateral acceleration, body and wheel velocity, as well as ride and damper 
height. Applying this information, the system acts directly on the anti-roll bar swivel motors and the electromagnetic valves in the dampers, varying 
body roll and the damping effect appropriately at all times and in all situations. 
Simply by pressing a button the driver is able to choose either a sporting 
or a comfortable setting on Adaptive Drive.

BMW Adaptive Drive uses high-speed FlexRay data transmission for fast 
and reliable coordination of data. This system, developed to serial production standard by a development consortium under the leadership of BMW, 
offers a an entirely new standard of data transfer capacity – and BMW is the 
first vehicle manufacturer in the world to use FlexRay technology in a serial production car. 

























5.	Driving experience:�Dynamic performance in �a new dimension.








4.	Design:�Elegant sportiness meets supreme presence.





3.	Concept:�A new vehicle category, a new driving experience.

















