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Technical Specifications.

BMW X5 xDrive35i, 
BMW X5 xDrive50i.

	
	
	BMW X5 xDrive35i
	
	BMW X5 xDrive50i

	
	
	
	
	

	Body
	
	
	
	

	Number of doors/seats
	
	5 / 5 (7) 1)
	
	5 / 5 (7) 1)

	Length/Width/Height (unladen)
	mm
	4857 / 1933 / 1776 2)
	
	4857 / 1933 / 1776 2)

	Wheelbase
	mm
	2933
	
	2933

	Track front/rear
	mm
	1644 / 1650
	
	1640 / 1646

	Turning cycle
	m
	12.8
	
	12.8

	Tank capacity
	appr ltr
	85
	
	85

	Cooling system incl. heating
	ltr
	10.9
	
	17.2

	Engine oil3)
	ltr
	6.5
	
	8.5

	Weight, unladen, to DIN/EU
	kg
	2070 / 2145


	
	2190 / 2265



	Max load to DIN
	kg
	680 (890) 1)
	
	680 (835) 1)

	Max perm weight, overall
	kg
	2750 (2960) 1)
	
	2870 (3025) 1)

	Max perm axle load front/rear
	kg
	1265 / 1550
(1270 / 1755) 1)
	
	1365 / 1570
(1370 / 1740) 1)

	Max perm trailer load (12 %)
braked/unbraked
	kg
	3500 / 750
	
	3500 / 750

	Perm roof load/trail download
	kg
	100/140
	
	100/140

	Luggage capacity
	ltr
	620-1750
	
	620-1750

	Air resistance
	cd x A
	0.33 x 2.87
	
	0.35 x 2.87

	
	
	
	
	

	Engine
	
	
	
	

	Config/no of cyls/valves
	
	R / 6 / 4
	
	V / 8 / 4

	Engine technology
	 
	BMW TwinPower Turbo, direct injection
(High Precision Injection), fully variable valve control (VALVETRONIC)
	
	BMW TwinPower Turbo, direct injection
(High Precision Injection)

	Capacity
	cc
	2979
	
	4395

	Stroke/bore
	mm
	89.6 / 84.0
	
	88.3 / 89.0

	Compression ratio
	:1
	10.2
	
	10.0

	Fuel grade
	
	at least RON 91
	
	at least RON 91

	Max output
	kW/bhp
	225 / 306
	
	300 / 407

	at
	rpm
	5800
	
	5500-6400

	Max torque
	Nm
	400
	
	600

	at
	rpm
	1200-5000
	
	1750-4500

	
	
	
	
	

	Electrical system
	
	
	
	

	Battery/installation
	Ah/–
	90 / luggage comp
	
	90 / luggage comp

	Alternator
	A/W
	210 / 2940
	
	210 / 2940

	
	
	
	
	

	Driving dynamics and safety
	

	Suspension, front
	
	Double-track control arm front axle, small, negative steering offset, anti-dive

	Suspension, rear
	
	Integral-IV rear axle, multi-dimensional suspension with 
anti-squat and anti-dive

	Brakes, front
	
	Single-piston floating-calliper disc brakes

	Diameter
	mm
	348 x 30 / vented
	
	385 x 36 / vented

	Brakes, rear
	
	Single-piston floating-calliper disc brakes

	Diameter
	mm
	320 x 20 / vented
	
	345 x 24 / vented

	Driving stability systems
	  
	Fitted as standard: DSC incl. ABS and DTC (Dynamic Traction Control), CBC Cornering Brake Control, DBC Dynamic Brake Control, rain brake support, 
fading compensation, hill-start assistant; DSC networked with xDrive four-wheel drive, adaptive brake compensation, HDC Hill Descent Control, 
optional: Adaptive Drive

	Safety features
	  
	Fitted as standard: Airbags for driver and front seat passenger, side airbags for driver and front seat passenger, head airbags for the first and second seat row, crash-active headrests at the front, three-point automatic belts on all seats, on the front seats with pretensioners, belt-force limiters and belt stoppers, crash sensors, roll-over sensors, tyre defect indicator

	Steering
	
	Rack-and-pinion power steering with Servotronic function, optional: Active Steering

	Overall steering transmission
	:1
	19.5
	
	19.5

	Tyres front/rear
	255/55 R18 109 V XL RSC
	
	255/50 R19 107W XL RSC

	Wheels front/rear
	
	8.5J x 18 LM
	
	9J x 19 LM


	
	
	BMW X5 xDrive35i
	
	BMW X5 xDrive50i

	
	
	
	
	

	BMW ConnectedDrive
	
	
	
	

	Comfort
	
	Optional extras: BMW Assist featuring, inter alia, information service, remote functions and traffic info+, BMW TeleServices, integration of mobile devices

	Infotainment
	
	Optional extras: Internet access, BMW Online featuring, inter alia, parking info, country-relevant info, Google search by type of business, news, weather, realtime, office functions, BMW Routes and online update of music tracks

	Safety
	
	Optional extras: Adaptive Cornering Headlights, High-beam Assistant, Park Distance Control, Side View, reversing camera with Surround View, Head-up Display, Cruise Control with Stop & Go function, Lane Departure Warning, Speed Limit Info, automatic/advanced emergency call

	
	
	
	
	

	Transmission
	
	
	
	

	Type
	
	8-speed automatic transmission with Steptronic

	Gear ratios
I
	:1
	4.714
	
	4.714

	                                  
II
	:1
	3.143
	
	3.143

	                                  
III
	:1
	2.105
	
	2.105

	                                  
IV
	:1
	1.667
	
	1.667

	                                  
V
	:1
	1.285
	
	1.285

	                                   
VI
	:1
	1.000
	
	1.000

	                                   
VII
	:1
	0.839
	
	0.839

	                                   
VIII
	:1
	0.667
	
	0.667

	                                   
R
	:1
	3.295
	
	3.317

	Final drive
	:1
	3.154
	
	3.154

	
	
	
	
	

	Performance
	
	
	
	

	Power-to-weight ratio
	kg/kW
	9.2
	
	7.3

	Output per litre
	kW/ltr
	75.5
	
	68.3

	Acceleration
0–100 km/h
	s
	6.8
	
	5.5

	
0–1000 m
	s
	27.0
	
	24.8

	in 4th/5th gear 80–120 km/h
	s
	-
	
	-

	Top speed
	km/h
	235
	
	240 (250) 4)

	
	
	
	
	

	Off-road characteristics
	
	
	
	

	Overhang angle
front/rear
	
°
	
25.5/22.7
	
	
25.5/22.7

	Ramp angle
	°
	19.8
	
	19.8

	Ground-clearance when unladen
	mm
	222
	
	222

	Wading depth (at 7 km/h)
	mm
	500
	
	500

	
	
	
	
	

	BMW EfficientDynamics
	
	
	
	

	BMW EfficientDynamics measures as standard
	
	Brake Energy Regeneration, demand-controlled ancillary components, map-controlled oil pump (BMW X5 xDrive35i) intelligent lightweight construction, air vent control (BMW X5 xDrive35i), disengageable a/c compressor, transfer box with optimized efficiency, tyres with reduced rolling resistance

	
	
	
	
	

	Fuel con in the EU cycle
	
	
	
	

	Urban
	ltr/100 km
	13.2
	
	17.5

	Extra-urban
	ltr/100 km
	8.3
	
	9.6

	Composite
	ltr/100 km
	10.1
	
	12.5

	CO2
	g/km
	236
	
	292

	Emission classification
	
	EU5  
	
	EU5  

	
	
	
	
	

	Insurance category (German)
	
	
	
	

	KH / VK / TK
	
	23 / 26 / 30
	
	23 / 29 / 30


Technical data valid for ACEA markets/Part of registration-specific data only apply to Germany (weights, top speed)

1) With optional third seat row

2) Height without roof aerial: 1,739 mm
3) Oil filling quantity

4) With optional high-speed tuning (market-specific)

BMW X5 xDrive30d, 
BMW X5 xDrive40d.

	
	
	BMW X5 xDrive30d
	
	BMW X5 xDrive40d

	
	
	
	
	

	Body
	
	
	
	

	Number of doors/seats
	
	5 / 5 (7) 1)
	
	5 / 5 (7) 1)

	Length/Width/Height (unladen)
	mm
	4857 / 1933 / 1776 2)
	
	4857 / 1933 / 1776 2)

	Wheelbase
	mm
	2933
	
	2933

	Track front/rear
	mm
	1644 / 1650
	
	1644 / 1650

	Turning cycle
	m
	12.8
	
	12.8

	Tank capacity
	appr ltr
	85
	
	85

	Cooling system incl. heating
	ltr
	10.4
	
	10.4

	Engine oil3)
	ltr
	7.5
	
	7.5

	Weight, unladen, to DIN/EU
	kg
	2075 / 2150


	
	2110 / 2185



	Max load to DIN
	kg
	680 (890) 1)
	
	680 (890) 1)

	Max perm weight, overall
	kg
	2755 (2965) 1)
	
	2790 (3000) 1)

	Max perm axle load front/rear
	kg
	1275 / 1545

(1280 / 1745) 1)
	
	1300 / 1555
(1305 / 1755) 1)


	Max perm trailer load (12 %)
braked/unbraked
	kg
	3500 / 750


	
	3500 / 750



	Perm roof load/trail download
	kg
	100/140
	
	100/140

	Luggage capacity
	ltr
	620-1750
	
	620-1750

	Air resistance
	cd x A
	0.34 x 2.87
	
	0.34 x 2.87

	
	
	
	
	

	Engine
	
	
	
	

	Config/no of cyls/valves
	
	R / 6 / 4
	
	R / 6 / 4

	Engine technology
	 
	Turbocharger with variable intake geometry, Common Rail direct injection with piezo injectors (max. injection pressure: 1800 bar)
	
	BMW TwinPower Turbo (Variable Twin Turbo), Common Rail direct injection with piezo injectors (max. injection pressure: 2000 bar)

	Capacity
	cc
	2993
	
	2993

	Stroke/bore
	mm
	90.0 / 84.0
	
	90.0 / 84.0

	Compression ratio
	:1
	16.5
	
	16.5

	Fuel grade
	
	Diesel
	
	Diesel

	Max output
	kW/bhp
	180 / 245
	
	225 / 306

	at
	rpm
	4000
	
	4400

	Max torque
	Nm
	540
	
	600

	at
	rpm
	1750-3000
	
	1500-2500

	
	
	
	
	

	Electrical system
	
	
	
	

	Battery/installation
	Ah/–
	90 / luggage comp
	
	90 / luggage comp

	Alternator
	A/W
	170 / 2380
	
	170 / 2380

	
	
	
	
	

	Driving dynamics and safety
	

	Suspension, front
	
	Double-track control arm, small, negative steering offset, anti-dive

	Suspension, rear
	
	Integral-IV rear axle, multi-dimensional suspension with 
anti-squat and anti-dive

	Brakes, front
	
	Single-piston floating-calliper disc brakes

	Diameter
	mm
	332 x 30 / vented
	
	348 x 30 / vented

	Brakes, rear
	
	Single-piston floating-calliper disc brakes

	Diameter
	mm
	320 x 20 / vented
	
	320 x 20 / vented

	Driving stability systems
	  
	Fitted as standard: DSC incl. ABS and DTC (Dynamic Traction Control), CBC Cornering Brake Control, DBC Dynamic Brake Control, rain brake support, 
fading compensation, hill-start assistant; DSC networked with xDrive four-wheel drive, adaptive brake compensation, HDC Hill Descent Control, 
optional: Adaptive Drive

	Safety features
	  
	Fitted as standard: Airbags for driver and front seat passenger, side airbags for driver and front seat passenger, head airbags for the first and second seat row, crash-active headrests at the front, three-point automatic belts on all seats, on the front seats with pretensioners, belt-force limiters and belt stoppers, crash sensors, roll-over sensors, tyre defect indicator

	Steering
	
	Rack-and-pinion power steering with Servotronic function, optional: Active Steering

	Overall steering transmission
	:1
	19.5
	
	19.5

	Tyres front/rear
	255/55 R18 109 H XL RSC
	255/55 R18 109 V XL RSC

	Wheels front/rear
	
	8.5J x 18 LM
	
	8.5J x 18 LM


	
	
	BMW X5 xDrive30d
	
	BMW X5 xDrive40d

	
	
	
	
	

	BMW ConnectedDrive
	
	
	
	

	Comfort
	
	Optional extras: BMW Assist featuring, inter alia, information service, remote functions and traffic info+, BMW TeleServices, integration of mobile devices

	Infotainment
	
	Optional extras: Internet access, BMW Online featuring, inter alia, parking info, country-relevant info, Google search by type of business, news, weather, realtime, office functions, BMW Routes and online update of music tracks

	Safety
	
	Optional extras: Adaptive Cornering Headlights, High-beam Assistant, Park Distance Control, Side View, reversing camera with Surround View, Head-up Display, cruise control with Stop & Go function, Lane Departure Warning, Speed Limit Info, automatic/advanced emergency call

	
	
	
	
	

	Transmission
	
	
	
	

	Type
	
	8-speed automatic transmission with Steptronic

	Gear ratios
I
	:1
	4.714
	
	4.714

	                                  
II
	:1
	3.143
	
	3.143

	                                  
III
	:1
	2.105
	
	2.105

	                                  
IV
	:1
	1.667
	
	1.667

	                                  
V
	:1
	1.285
	
	1.285

	                                   
VI
	:1
	1.000
	
	1.000

	                                   
VII
	:1
	0.839
	
	0.839

	                                   
VIII
	:1
	0.667
	
	0.667

	                                   
R
	:1
	3.317
	
	3.317

	Final drive
	:1
	3.154
	
	3.154

	
	
	
	
	

	Performance
	
	
	
	

	Power-to-weight ratio
	kg/kW
	11.5
	
	9.4

	Output per litre
	kW/ltr
	60.1
	
	75.2

	Acceleration
0–100 km/h
	s
	7.6
	
	6.6

	
0–1000 m
	s
	28.5
	
	27.0

	in 4th/5th gear     80–120 km/h
	s
	-
	
	-

	Top speed
	km/h
	210 (222) 4)
	
	236

	
	
	
	
	

	Off-road characteristics
	
	
	
	

	Overhang angle
front/rear
	
°
	
25.5/22.7
	
	
25.5/22.7

	Ramp angle
	°
	19.8
	
	19.8

	Ground-clearance when unladen
	mm
	222
	
	222

	Wading depth (at 7 km/h)
	mm
	500
	
	500

	
	
	
	
	

	BMW EfficientDynamics
	
	
	
	

	BMW EfficientDynamics measures as standard
	
	Brake Energy Regeneration, demand-controlled ancillary components, map-controlled oil pump (BMW X5 xDrive35i) intelligent lightweight construction, air vent control (BMW X5 xDrive35i), disengageable a/c compressor, transfer box with optimized efficiency, tyres with reduced rolling resistance

	
	
	
	
	

	Fuel con in the EU cycle
	
	
	
	

	Urban
	ltr/100 km
	8.7
	
	8.8

	Extra-urban
	ltr/100 km
	6.7
	
	6.8

	Composite
	ltr/100 km
	7.4
	
	7.5

	CO2
	g/km
	195
	
	198

	Emission classification
	
	EU5  
	
	EU5  

	
	
	
	
	

	Insurance category (German)
	
	
	
	

	KH / VK / TK
	
	24 / 29 / 30
	
	24 / 29 / 30


Technical data valid for ACEA markets/Part of registration-specific data only apply to Germany (weights, top speed)

1) With optional third seat row

2) Height without roof aerial: 1,739 mm

3) Oil filling quantity

4) With optional high-speed tuning (market-specific)

BMW X5 M.

	
	
	BMW X5 M
	
	

	
	
	
	
	

	Body
	
	
	
	

	Number of doors/seats
	
	5 / 5
	
	

	Length/Width/Height (unladen)
	mm
	4851 / 1994 / 17641)
	
	

	Wheelbase
	mm
	2933
	
	

	Track front/rear
	mm
	1660 / 1672
	
	

	Turning cycle
	m
	12.8
	
	

	Tank capacity
	appr ltr
	85
	
	

	Cooling system incl. heating
	ltr
	17.0
	
	

	Engine oil3)
	ltr
	8.5
	
	

	Weight, unladen, to DIN/EU
	kg
	2305 / 2380


	
	

	Max load to DIN
	kg
	600
	
	

	Max perm weight, overall
	kg
	2905
	
	

	Max perm axle load front/rear
	kg
	1400 / 1560
	
	

	Max perm trailer load (12 %)
braked/unbraked
	kg
	3000 / 750
	
	

	Perm roof load/trail download
	kg
	100/120
	
	

	Luggage capacity
	ltr
	620 – 1750
	
	

	Air resistance
	cd x A
	0.38 x 2.90
	
	

	
	
	
	
	

	Engine
	
	
	
	

	Config/no. of cyls/valves
	
	V90/ 8 / 4
	
	

	Engine technology
	 
	M TwinPower Turbo with Cylinder-bank Comprehensive Manifold and Twin Scroll Twin Turbo technology, petrol direct injection
 (High Precision Injection), Double Vanos
	
	

	Capacity
	cc
	4395
	
	

	Stroke/bore
	mm
	88.3 / 89.0
	
	

	Compression ratio
	:1
	9.3
	
	

	Fuel grade
	
	 at least RON 95
	
	

	Max power
	kW/bhp
	408 / 555
	
	

	at
	rpm
	6000
	
	

	Max torque
	Nm
	680
	
	

	at
	rpm
	1500 – 5650
	
	

	
	
	
	
	

	Electrical system
	
	
	
	

	Battery/installation
	Ah/–
	90 / luggage comp
	
	

	Alternator
	A/W
	210 / 2940
	
	

	
	
	
	
	

	Driving dynamics and safety
	

	Suspension, front
	
	Double-track control arm front axle with M specific elasto-kinematics, small, negative steering roll radius, anti-dive

	Suspension, rear
	
	Integral-IV rear axle with M specific elasto-kinematics, multi-dimensional suspension, anti-squat and anti-dive, self-levelling air suspension

	Brakes, front
	
	Four-piston fixed-calliper disk brakes
	
	

	Diameter
	mm
	395 x 36 / vented
	
	

	Brakes, rear
	
	One-piston floating-calliper disk brakes
	
	

	Diameter
	mm
	385 x 24 / vented
	
	

	Driving stability systems
	  
	Fitted as standard: DSC incl. ABS and M Dynamic Mode, CBC Cornering Brake Control, DBC Dynamic Brake Control, ADB-X Automatic Differential Brake, rain brake support, fading compensation, hill-start assistant; DSC networked with xDrive four-wheel drive, Dynamic Performance Control, HDC Hill Descent Control, Adaptive Drive

	Safety features
	  
	Fitted as standard: Airbags for driver and front seat passenger, side airbags for driver and front seat passenger, head airbags for the first and second seat row, crash-active headrests at the front, three-point automatic belts on all seats, on the front seats with pretensioners, belt-force limiters and belt stoppers, crash sensors, roll-over sensors, tyre defect indicator

	Steering
	
	Rack-and-pinion power steering with M specific Servotronic function

	Overall steering transmission
	:1
	19.5
	
	

	Tyres front/rear
	
	275/40 R20 106Y XL RSC / 315/35 R20 110Y XL RSC
	
	

	Wheels front/rear
	
	10J x 20 LM / 11J x 20 LM
	
	


	
	
	BMW X5 M
	
	

	
	
	
	
	

	BMW ConnectedDrive
	
	
	
	

	Comfort
	
	Optional extras: BMW Assist featuring, inter alia, information service, remote functions and traffic info+, BMW TeleServices, integration of mobile devices

	Infotainment
	
	Optional extras: Internet access, BMW Online featuring, inter alia, parking info, country-relevant info, Google search by type of business, news, weather, realtime, office functions, BMW Routes and online update of music tracks

	Safety
	
	Fitted as standard: Adaptive Cornering Headlights, Park Distance Control, Head-Up-Display, Cruise Control with brake function, 
optional: reversing camera with Top View, Side View, High-beam assistant, 
Speed Limit Info, automatic/advanced emergency call

	
	
	
	
	

	Transmission
	
	
	
	

	Type
	
	M Sport six-speed automatic gearbox with Steptronic, electronic
gearshift selector and shift paddles on the steering wheel

	Gear ratios
I
	:1
	4.171
	
	

	                                  
II
	:1
	2.340
	
	

	                                  
III
	:1
	1.521
	
	

	                                  
IV
	:1
	1.143
	
	

	                                  
V
	:1
	0.867
	
	

	                                   
VI
	:1
	0.691
	
	

	                                   
R
	:1
	3.403
	
	

	Final drive
	:1
	3.909
	
	

	
	
	
	
	

	Performance
	
	
	
	

	Power-to-weight-ratio
	kg/kW

	5.6


	
	

	Output per litre
	kW/ltr
	92.8
	
	

	Acceleration
0–100 km/h
	s
	4.7
	
	

	
0–200 km/h
	s
	16.9
	
	

	
0–1000 m
	s
	23.5
	
	

	in 4th/5th gear
80–120 km/h
	s
	4.3 / 5.1
	
	

	Top speed
	km/h
	250 (275)3)
	
	

	
	
	
	
	

	Off-road characteristics
	
	
	
	

	Overhang angle
front/rear
	
°
	
22 / 21.5
	
	


	Ramp angle
	°
	18.6
	
	

	Ground-clearance when unladen
	mm
	207
	
	

	
	
	
	
	

	BMW EfficientDynamics
	
	
	
	

	BMW EfficientDynamics measures as standard
	
	Brake Energy Regeneration, demand-controlled ancillary components, intelligent lightweight construction, disengageable air-conditioning compressor, Dynamic Stability Control with demand-responsive pump control

	
	
	
	
	

	Fuel con in the EU cycle
	
	
	
	

	Urban
	ltr/100 km
	19.3
	
	

	Extra-urban
	ltr/100 km
	10.8
	
	

	Composite
	ltr/100 km
	13.9
	
	

	CO2
	g/km
	325
	
	

	Emission classification
	
	EU5  
	
	

	
	
	
	
	

	Insurance category (German)
	
	24 / 32 / 31
	
	

	KH / VK / TK
	
	
	
	


Technical data valid for ACEA markets/Part of registration-specific data only apply to Germany (weights, top speed)

1)  Height without roof aerial: 1,726 mm

2)  Oil filling quantity

3)  In conjunction with optional M Driver’s Package

