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Specifications BMW X5.
X5 xDrive35i, X5 xDrive50i
	
	
	BMW X5 xDrive35i
	
	BMW X5 xDrive50i

	
	
	
	
	

	Body
	
	
	
	

	No of doors / seats      
	
	5 / 5 (7) 1)
	
	5 / 5 (7) 1)

	Length/width/height (unladen)
	mm
	4857 / 1933 / 1776 2)
	
	4857 / 1933 / 1776 2)

	Wheelbase
	mm
	2933
	
	2933

	Track, front/rear      
	mm
	1644 / 1650
	
	1640 / 1646

	Turning circle
	m
	12.8
	
	12.8

	Tank capacity
	app ltr
	85
	
	85

	Cooling system incl heater
	ltr
	10.9
	
	17.2

	Engine oil3)
	ltr
	6.5
	
	8.5

	Weight, unladen, to DIN/EU
	kg
	2070 / 2145


	
	2190 / 2265



	Max load to DIN
	kg
	680 (890) 1)
	
	680 (835) 1)

	Max permissible  
	kg
	2750 (2960) 1)
	
	2870 (3025) 1)

	Max axle load, front/rear   
	kg
	1265 / 1550
(1270 / 1755) 1)
	
	1365 / 1570
(1370 / 1740) 1)

	Max trailer load (12%)
braked/unbraked   
	kg
	3500 / 750
	
	3500 / 750

	Max roofload/max towbar downl 
	kg
	100/140
	
	100/140

	Luggage comp capacity 
	ltr
	620-1750
	
	620-1750

	Air drag       
	cd x A
	0.33 x 2.87
	
	0.35 x 2.87

	
	
	
	
	

	Power Unit
	
	
	
	

	Config/No of cyls/valves     Zylinder/Ventile


	
	Straight-6 / 4
	
	V / 8 / 4

	Engine technology
	 
	BMW TwinPower Turbo, direct fuel injection
(High Precision Injection), fully variable,

valve management

(VALVETRONIC)
	
	BMW TwinPower Turbo, direct fuel injection 

(High Precision Injection)

	Capacity, effective
	cc
	2979
	
	4395

	Stroke / bore 
	mm
	89.6 / 84.0
	
	88.3 / 89.0

	Compression ratio
	:1
	10.2
	
	10.0

	Fuel       
	
	min RON 91
	
	min RON 91

	Max output
	kW/hp
	225 / 306
	
	300 / 407

	at
	rpm
	5800
	
	5500-6400

	Max torque
	Nm/lb-ft
	400 / 295
	
	600 / 442

	at
	rpm
	1200-5000
	
	1750-4500

	
	
	
	
	

	Electrical System
	
	
	
	

	Battery/location  
	Ah/–
	90 / luggage comp
	
	90 / luggage comp

	Alternator
	A/W
	210 / 2940
	
	210 / 2940

	
	
	
	
	

	Driving Dynamics and Safety
	

	Suspension, front  
	
	Double wishbone axle, small, negative steering roll radius, anti-dive 

	Suspension, rear    
	
	Integral-IV rear axle, multi-dimensional suspension with anti-squat and anti-dive

	Brakes, front 
	
	Single-piston swing-calliper disc brakes

	Diameter  
	mm
	348 x 30 / vented  
	
	385 x 36 / vented  

	Brakes, rear 
	
	Single-piston swing-calliper disc brakes

	Diameter  
	mm
	320 x 20 / vented  
	
	345 x 24 / vented  

	Driving stability systems
	  
	Standard: DSC incl ABS and DTC (Dynamic Traction Control), CBC Cornering, Brake Control, DBC Dynamic Brake Control, Dry Braking, 

Fading Compensation, Start-Off Assistant, DSC networked to xDrive all-wheel drive, Dynamic Brake Compensation, HDC Hill Descent Control,

optional:Adaptive Drive

	Safety equipment        
	  
	Standard: airbags for driver and front passenger, side airbags for driver and front passenger, head airbags on the first and second row of seats, crash-activated headrests at the front, three-point inertia-reel belts on all seats, with belt latch tensioner, belt force limiter and belt retainer at the front, rash sensors, roll-over sensors, Tyre Defect Indicator 

	Steering 
	
	Rack-and-pinion power steering with Servotronic, optional: Active Steering

	Steering transmission, overall
	:1
	19.5
	
	19.5

	Tyres, front/rear  
	
	255/55 R18 109H XL RSC
	
	255/50 R19 107W XL RSC

	Rims, front/rear  
	
	8.5J x 18 light-alloy
	
	9J x 19 light-alloy


Specifications BMW X5.
	
	
	BMW X5 xDrive35i
	
	BMW X5 xDrive50i

	
	
	
	
	

	BMW ConnectedDrive
	
	
	
	

	Comfort
	
	Optional: BMW Assist incl Enquiry Service, remote control function and V-Info+, BMW TeleServices, integration of mobile terminals

	Infotainment
	
	Optional: access to the internet, BMW Online incl Parkinfo, National Info, Google directory search, news, realtime weather, office functions, BMW Routes and online music update

	Safety    
	
	Optional: Adaptive Headlights with Bending Lights, High-Beam Assistant, Park  Distance Control, Side View, back-up camera withTop View, Head-Up Display, Cruise Control with Stop & Go, Lane Departure Warning, Speed Limit Info, Automatic/Enhanced Emergency Call     

	
	
	
	
	

	Transmission
	
	
	
	

	Type of transmission
	
	Eight-speed automatic with Steptronic   

	Gear ratios
I
	:1
	4.714
	
	4.714

	                                  
II
	:1
	3.143
	
	3.143

	                                  
III
	:1
	2.105
	
	2.105

	                                  
IV
	:1
	1.667
	
	1.667

	                                  
V
	:1
	1.285
	
	1.285

	                                   
VI
	:1
	1.000
	
	1.000

	                                   
VII
	:1
	0.839
	
	0.839

	                                   
VIII
	:1
	0.667
	
	0.667

	                                   
Reverse
	:1
	3.295
	
	3.317

	Final drive           
	:1
	3.154
	
	3.154

	
	
	
	
	

	Performance  
	
	
	
	

	Power-to-weight ratio            
	kg/kW
	9.2
	
	7.3

	Output per litre
	kW/hp
	75.5/102.7
	
	68.3/92.9

	Acceleration
0–100 km/h
	sec
	6.8
	
	5.5

	                           standing-start km
	sec
	27.0
	
	24.8

	in 4th/5th gear      80–120 km/h
	sec
	-
	
	-

	Top speed            
	km/h
	235
	
	240 (250) 4)

	
	
	
	
	

	Offroad Features
	
	
	
	

	Overhang angle,
front/rear
	
°
	
25.5/22.7
	
	
25.5/22.7

	Ramp angle
	°
	19.8
	
	19.8

	Ground clearance, unladen
	mm
	222
	
	222

	Water depth (at 7 km/h)
	mm
	500
	
	500

	
	
	
	
	

	BMW EfficientDynamics
	
	
	
	

	BMW EfficientDynamics standard features    
	
	Brake Energy Regenereation, on-demand control of ancillary units, map-controlled oil pump (BMW X5 xDrive35i), intelligent lightweight construction, air flap control (X5 xDrive35i), a/c compressor detachable, tyres with reduced roll resistance

	
	
	
	
	

	Fuel consumption in EU Cycle
	
	
	
	

	Urban   
	l/100 km
	13.2
	
	17.5

	Extra-urban   
	l/100 km
	8.3
	
	9.6

	Combined 
	l/100 km
	10.1
	
	12.5

	CO2
	g/km
	236
	
	292

	Emission rating      
	
	EU5  
	
	EU5  

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	


Specifications apply to ACEA markets/homologation-relevant data applicable in part only to Germany (weight, top speed)

1) With optional third row of seats

2) Height without roof aerial 1739 mm

3) Oil change    

4) With optional high speed set-up (depending on market)




















































