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2006 BMW Z4 ROADSTER
Product Highlights

Z4 Roadster 3.0i & Z4 Roadster 3.0si

General

•
Series of 2-seater Roadsters, introduced in model year 2003; major evolution for 2006

•
Available in two new models: Z4 Roadster 3.0i at $36,295 base price including destination and handling; Z4 3.0i at $42,795

•
Built at BMW’s Spartanburg, South Carolina production plant

What’s new for 2006

As of 5/05 production, actually during ’05 model year:

•
General re-calibration of suspension to enhance both handling and riding comfort
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As of 1/06 production:

Performance & efficiency

•
All-new, more powerful N52 engines for both models –


•
Magnesium/aluminum composite construction


•
Valvetronic variable intake-valve lift


•
Electric water pump


•
Volume-controlled oil pump

What’s new – performance & efficiency (cont.)


•
3.0i model – 215 hp/185 lb-ft. torque vs. former 2.5i’s 184 hp/175 lb-ft.


•
3.0si model – 255 hp/220 lb-ft. torque vs. former 3.0i’s 225 hp/214 lb-ft.

•
New final drive ratios, numerically higher to further improve acceleration

•
6-speed manual transmission now standard on both models (former 2.5i model had a 5-speed)

•
6-speed automatic transmission optional on both models (formerly 5-speed), with new features:


•
Shift paddles on steering wheel


•
Direct Selection of Manual shift mode via paddle downshift 


•
Sportier overall programming

Handling, ride & braking

•
17-in. wheels and tires now standard on both models, new 17-in. differentiated front/rear sizes as part of 3.0i Sport Package, new wheel designs throughout:


•
3.0i standard – 17 x 8.0 wheels, 225/45R-17 tires 


•
3.0i Sport Package – 17 x 8.0 front/17 x 8.5 rear wheels with 225/45 front / 245/40 rear tires 1


•
3.0si standard – 17 x 8.0 wheels, 225/45R-17 tires 1


•
3.0si Sport Package – 18 x 8.0 front/18 x 8.5 rear wheels, 225/40 front / 255/35 rear tires 1

•
Dynamic Stability Control system incorporates new braking functions –


•
Brake Fade Compensation


•
Brake Standby


•
Brake Drying


•
Start-off Assistant


•
Modulated ABS function, for smoother operation

What’s new (cont.)

Exterior design & function

•
New front bumper ensemble, with larger air intake, rectangular foglights and enhanced integration with body lines

•
Front side reflectors, formerly part of wraparound lighting clusters, now set into surface of wheel openings

•
New wheel designs for all four wheel/tire configurations

•
New rear bumper/apron ensemble

•
New taillight design

•
Stainless-steel exhaust tips (3.0si only)

•
New metallic paint colors

Ergonomics, luxury & convenience

•
New interior colors:


•
Active Sport cloth/leather (3.0i only) – new blue and black schemes


•
Oregon leather (optional 3.0i, standard 3.0si) – Pearl Gray added to existing three schemes


•
New England leather (optional 3.0si only) with more extensive leather – Saddle Brown added to existing three schemes

•
Glove compartment: silicon damper for smoother opening/closing, also now illuminated

•
New aluminum interior trim, horizontal brushed

•
Rubber mat at bottom of door pockets

•
Steering-wheel spokes now trimmed in galvanic material in all versions

•
New shift knob for automatic transmission

•
Automatic climate control (optional 3.0i, standard 3.0si) has new materials on rotary knobs: galvanic trim for enhanced appearance, rubber surfaces for improved tactile feel

•
Adjusting wheels for air vents also have rubber touch tactile surfaces

Options

•
Headlight cleaning system newly optional

•
Alternate wood trim, Dark Poplar Grain (Light Poplar Grain continues)

•
New wheels in Sport Packages, described above

Z4 Series Key Features

Performance & efficiency features

•
3.0-liter DOHC 24-valve inline 6-cylinder engine with Valvetronic variable intake-valve lift and Double VANOS 
 steplessly variable valve timing: 215 (3.0i) or 255 hp (3.0si)

•
Choice of 6-speed manual transmission or 6-speed STEPTRONIC automatic transmission

Handling, ride & braking features

•
High-rigidity roadster body/chassis unit with aluminum hood

•
Strut-type front suspension with forged-aluminum lower arms

•
Central Link rear suspension with cast-aluminum upper transverse links

•
Vehicle-speed-sensitive electric power steering

•
4-wheel ventilated disc brakes

•
Dynamic Stability Control (traction and stability system)

•
Run-flat performance tires on all versions

•
Flat Tire Monitor standard

•
Generously dimensioned wheels and tires, 17- or 18-in.

Exterior & aerodynamics features

•
Unique Roadster design, featuring interplay of convex and concave surfaces, traditional and contemporary style elements

•
Adaptive Brake Lights (illumination increases with harder braking)

•
Rain-sensing windshield wipers

•
Front foglights

•
Heated exterior mirrors and windshield-washer jets

•
Easy-to-operate manual softtop with heated glass rear window

•
Model identifying script on front flanks

Ergonomics, luxury & convenience features

•
Vehicle and Key Memory

•
Keyless entry with multi-function remote

•
Dual power exterior mirrors

•
Automatic headlight control (switches on headlights and related lighting when ambient light drops below a certain level)

Z4 Series key features – ergonomics, luxury & convenience (cont.)

•
Leather-covered tilt/telescopic sport steering wheel with fingertip audio controls

•
Cruise control

•
6-way adjustable sport seats

•
Outside-temperature display

•
Power windows with 1-touch open/close, power sealing system

•
Manual climate control with microfilter ventilation standard in 3.0i model; automatic climate control optional in 3.0i, standard in 3.0si

•
Anti-theft AM/FM/CD audio system with Radio Data System, 10 speakers

•
Pre-wiring for phone and CD changer

•
Variable softtop compartment

Safety & security

•
Front-impact Supplementary Restraint System with 2-stage Smart Airbags

•
Automatic safety-belt tensioners and force limiters

•
Active Knee Protection

•
LATCH attachment for child-restraint safety seat

•
Passenger-airbag de-activation switch and indicator

•
Side-impact airbags

•
Rollover Protection

•
Battery Safety Terminal

•
Central locking system

•
Coded Driveaway Protection (immobilizer system)

•
Pre-wiring for alarm system

Factory-installed options
•
Premium and Sport Packages available for each model

•
Sport Packages include Dynamic Driving Control, with Sport button for selecting Sport mode

•
6-speed STEPTRONIC automatic transmission

•
Metallic paint

•
Xenon headlights with auto-leveling

•
Headlight cleaning system

•
Fully automatic power softtop

•
Wide range of upholstery and interior trim options

Factory-installed options (cont.)
•
8-way power seats with driver’s-seat memory

•
M sport seats

•
Heated seats

•
On-board Computer (3.0i only; standard 3.0si)

•
On-board Navigation System with DVD database

•
Premium Sound System, THX Certified (3.0i only; standard 3.0si)

•
Preparation for removable hardtop

•
BMW Assist, including Bluetooth cellphone interface
BMW center-installed accessories

•
Removable hardtop

•
Alarm system

•
Sirius Satellite Radio

•
iPod adapter kit

•
6-disc CD changer

•
Wind deflector

•
Trunk storage system

•
Trunk-mount carrier rack and accessories

…and more
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� – Due to low-profile tires, please note: Wheels, tires and suspension parts are more susceptible to road hazard and consequential damages. Z4 models are not equipped with a spare tire and wheel. Performance tires are not recommended for driving in snow and ice conditions.


� – VANOS = VAriable NOckenwellen Steuerung = variable camshaft control, or variable valve timing.
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