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BMW 뉴 Z4 3.0si 쿠페 제원표


	Body
	
	Z4 Coupé 3.0si
	
	

	도어/시트 수
	
	2/2
	
	

	전장/전폭/전고
	mm
	4,091/1,781/1,268
	
	

	휠베이스
	mm
	2,495
	
	

	트랙, 앞/뒤
wgsdfg


	mm
	1,473/1,523
	
	

	회전 반경
	m
	9.8
	
	

	연료탱크용량
	ltr appr.
	55
	
	

	냉각시스템 (히팅 포함)
l
	ltr
	7.6 (8.4)
	
	

	엔진 오일
Getriebeöl


	ltr
	6.5
	
	

	변속기/리어 액슬 오일
	ltr
	lifetime filling
	
	

	공차중량
	kg
	1,350
	
	

	최대적재중량 (DIN)
	kg
	330
	
	

	수화물 적재용량 (VDA)
	ltr
	285–340
	
	

	공기저항계수
	cX x A
	0.34 x 1.91
	
	

	Engine
	
	
	
	

	레이아웃/실린더수/밸브수 
	
	Inline/6/4
	
	

	배기량
	cm³
	2,996
	
	

	보어/스트로크
	mm
	85.0/88.0
	
	

	압축비 
	:1
	10.7
	
	

	연료등급 3
	RON
	91–98
	
	

	최고출력
	hp/kW/min–1
	265/195/6,600
	
	

	최대토크
	Nm/min–1
	315/2,500
	
	

	Electrics
	
	
	    
	

	배터리/위치
	Ah/–
	55/engine comp
	
	

	발전기
	A/W
	155/2,170
	
	

	Chassis
	
	
	
	

	프론트 서스펜션
	
	Single-joint spring strut axle with multiple track control arms; 
fixed position ball joint on guide joint, thrust plate,
	
	

	
	
	twin-sleeve gas pressure spring struts; anti-squat and anti-dive
	
	

	리어 서스펜션
	
	Central arm axle with separate springs/dampers, twin-sleeve gas pressure dampers; anti-dive
	
	

	프론트 브레이크
	
	Disks


	
	

	직경
	mm
	325 x 25, vented
	
	

	리어 브레이크
	
	Disks


	
	

	직경
	mm
	294 x 19, vented 
	
	

	주행안전장치
	
	ABS, DSC, DTC
	
	

	스티어링 형식
	
	Electric power steering (EPS); rack&pinion steering
	
	

	스티어링 기어비
	:1
	16.0
	
	

	변속기 타입
	
	6 Speed 스텝트로닉)
	
	

	기어비
                    I
	:1
	4.17 
	
	

	

II
	:1
	2.34 
	
	

	

III
	:1
	1.52 
	
	

	

IV
	:1
	1.14 
	
	

	

V
	:1
	0.87 
	
	

	

VI
	:1
	0.69 
	
	

	후진 기어비
	:1
	3.40
	
	

	최종감속비
	:1
	3.64
	
	

	타이어
	
	225/45 
	
	

	휠
	
	8 J x 17 Cast Alu
	
	

	Performance
	
	
	
	

	가속도          
0–100km/h
	s
	6.0
	
	

	                           
0–1000 m
	s
	25.3
	
	

	최고속도4
	km/h
	250
	
	

	정부공인표준연비
Fuel consumption (EU cycle)
	km/l
	
	10.0
	
	

	CO2 
	g/km
	216
	
	

	Miscellaneous
	
	
	
	

	Emission level
	
	EU4
	
	


Numbers in ( ) for automatic transmission.


Weight of the car in road trim (DIN) plus 75 kg for driver and luggage.

2Deviations are possible under certain conditions.

3For Performance and fuel cunsumption figures: RON 98.
4Electronically limited.

BMW 뉴 Z4 3.0si 쿠페 토크 및 출력 곡선[image: image1.png]400

360

320

280

240

200

160

120

80

N
-,

Torque [Nm]

)

195 kW @

6600 min ]

200

180

315 Nm @

2750 min ]

160

N\

140

120

100

80

60

40

20

0 1000

Engine speed [min~

"

2000

3000

4000

5000

6000

0
7000

Output [KW]



.

BMW 뉴 Z4 3.0si 쿠페 외관 및 인테리어[image: image2.png]
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