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The wheels of time.

From wooden bikes to high-tech machines /

the new generation of BMW bikes.
Munich. Baden forestry official Baron Karl von Drais could certainly never have dreamt it. When he invented the “Draisine” bicycle in 1817, he had no idea that his means of propulsion would progress to become the most commonly-built machine in the world. Around a billion bicycles a year are produced worldwide, whereas only half that number of cars is manufactured. But from the wooden bike to the high-tech machines we have today, it’s been a long journey.

In early 19th century, the invention of the bicycle caused a real stir. Carl von Drais is reported to have taken only one hour to cover the stretch from his hometown of Mannheim to Schwetzingen, a distance of just under 15 kilometres, whereas the mail coach took almost four times as long to travel the same distance. So it’s no wonder that the wooden invention quickly caught on. However, actually riding the bike was a far from enjoyable experience. Poor roads made trundling along on wooden wheels very unpleasant, and the cyclist was constantly being jolted. Because so many Draisine riders were switching to the pavement, the police soon came up with the first fines: for illegal cycling on the pavement. 
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Even this could not dampen the rise to glory of the new means of propulsion, even if it was to take almost forty years before the Draisine became a proper bicycle, with a simple construction. 1861 was the year in which the “Vélocipède” was born, in which the front wheel was driven with a crank handle. With each press of the pedal, the wheel moved one revolution forwards. In England, the idea was born in 1870 of making the front wheel bigger, in order to enable the bike to go faster. Wheel diameters of up to 1.5 metres meant that cyclists could travel at speeds of up to 40 kilometres an hour. But this often led to serious accidents and injuries. Riding what was known as the Penny Farthing was a question of courage and skill. And even then, there were ‘extreme bikers’. The American John Stevens first crossed America in 1884 on a Penny Farthing, and then decided to continue his epic journey. For two years, he cycled around the world, travelling 20,000 kilometres across the continents. And since he also crossed the Rocky Mountains, Stevens is also unofficially the first mountainbiker.

The chain drive revolution

If Stevens had set off just one year later, his journey would have been considerably quicker and more comfortable. John Kemp Starley from England was the first to come up with the idea in 1885 of making the front and rear wheels the same size and propelling the ensemble with gears and a chain. The prototype of the present-day bicycle was born. The “Rover Safety Bicycle” thus offered a pleasant sitting position and made cycling a safe affair. In contrast to its predecessors, the Rover’s frame was no longer made from solid iron or hollow steel. Instead, Starley used an innovation from the Mannesmann brothers in Germany – namely seamless steel tubing.

The first ball bearings, which significantly reduce the friction between the hub and the crank bearing, brought a new dimension of comfort to cycling, and a short time later air-filled tyres were invented by John Boyd Dunlop. His first “tyres” were fashioned from a garden hose patched up with linen. Two years later, the Michelin brothers perfected Dunlop’s invention and patented the removable air-filled tyres. So cyclists could now also repair flat tyres on the move. The time was now right for real challenges. 1903 saw the first ever Tour de France. Frenchman Maurice Garin won, covering 2,426 kilometres. And not a gear change in sight, remember. It was only from 1932 onwards that race cyclists were permitted to stop and switch the chain manually to the second sprocket wheel. The invention of the derailleur wasn’t far behind, and the first racing derailleur gears, invented by Fichtel & Sachs, were launched onto the market in 1934. At around the same time, the German immigrant Ignaz Schwinn was developing a bicycle with inflatable tyres, known as the “Schwinn Excelsior”.

Without the inventor being aware of it, he’d created the forerunner of the mountainbike: sturdy and long-lasting wheels that offered a comfortable sitting position.

Rebuilding on two wheels

During and after the Second World War, bicycles were greatly treasured as a way of moving around and transporting goods. There were very few cars, let alone petrol. The manufacture of engines in German factories was forbidden by the Allies. For the Bayerische Motorenwerke in Munich, this meant switching to manufacturing other products. Instead of cars and motorbikes, other important products left the factories, including farming equipment, cooking pots – and bicycles. In 1950, the German Patent Office issued an official document for BMW with the number 800064. “The bicycle frame is identified by the fact that the main part of the frame is manufactured as a continuous moulded part from lightweight metal”, says the patent letter, describing the invention from Munich. Meanwhile, the production of cars and motorbikes was once again in full swing, so the plans for bicycle designs were temporarily shelved. Growing wealth and the range of motorised vehicles available quickly pushed the bicycle in Europe off its top spot as an everyday means of transport. It was only in the 1970s, during the fitness boom and as a consequence of jammed roads that the bike began to win back some of its appeal and importance. 

The Repack race sows the seed for an entire movement

Apart from those in the field of competitive racing, nobody gave a second thought to ascending mountains on bikes in the 1970s. With a weight of around 20 kilograms for a regular road bike and imprecise gears, it was really something that barely bore thinking about back then. But people were thinking about ascending mountains – at least the people who were crazy enough to try it. The American cycling enthusiasts Gary Fisher, Joe Breeze and Charles Kelly were three such people. Near San Francisco, they sped along the gravel paths of the 850-metre-high Mount Tamalpais, for fun. Their driving machines were old Schwinn bikes from the 1930s, with curved frame tubes and inflatable tyres. With just a back-pedal brake and no gears, the race was tantamount to a suicide mission too. Broken frames, handlebars and even snapped forks were soon a daily occurrence, so the demand for spare parts for the “clunker”, as it was known, soon escalated.

In 1976, the trio staged the first downhill race in history, on Fairfax’s local mountain. The three kilometre-long Cascade Canyon Fire Road demanded everything from the drivers and their bikes. During the descent, the back-pedal brakes became so hot that the grease ran out of the hub and had to be replaced

before the next race. This “repacking” quickly gave the race its name – the Repack race. 

Unhappy with their existing materials, Gary and the other members of the group tinkered around constantly with improvements: they borrowed the handlebars from the motorbike, and instead of the back-pedal brake, drum brakes were used on both wheels. The braking lever and cable were also copied from the world of motorbikes, and in particular from the German manufacturer Magura. At first viewed with scepticism, the derailleur system that Gary had pioneeringly screwed onto his clunker bike was ultimately copied with great enthusiasm. But each improvement of the parts was just fine-tuning. What was missing was the fundament. A new frame had to be built, one designed specially for crossing terrain. Based on plans drawn up by Gary Fisher, Tom Ritchey built a new bike that the pair, together with Charlie Kelly, wanted to market via their own company. The new bike forge was born and christened MountainBike.

A trend takes hold

Within a very short space of time, the mountain-biking ‘bug’ started to take hold. Major manufacturers started noticing the trend and series-producing the mountainbikes that Tom Ritchey had made by hand. The mountain-bikers also cribbed a further new feature from BMX bikes – aluminium wheel rims. At a stroke, the bikes became up to two kilograms lighter. 1982 was the year for the Japanese firm Shimano. It was the first company to launch gear components designed specially for mountainbikes onto the market. Its components were marketed as the legendary XT series. Its rivals initially poured nothing but scorn on Shimano, but they were soon laughing on the other side of their faces: Shimano evolved into the undisputed world market leader for gear components. The firm’s rise to success was not without hiccups, however. The oval-shaped “Biopace” chain wheel, invented in 1983 to make setting off easier, was a complete waste of effort and quickly disappeared from the market. At the end of the 1980s, two new products revitalised the market: Shimano was facing competition from the American manufacturer Sram with its Grip-Shift gear system, and Rockshox developed the first sprung fork, the RS-1. And a short time later in Germany, an old adversary made a move to gain market leadership for hydraulic brakes. Magura was back. 

In 1992, BMW decided to include a further mobility product in its portfolio. The Active and Dynamic Bike from Montegue was characterised by a very special feature: their folding mechanism allowed them to fit comfortably in any car boot. In the mid-90s, Easter and Christmas all came on one day for hardcore bikers, when Manitou unveiled the first frame with front and rear wheel suspension.

BMW took up this development in 1996, and announced its second bicycle patent since 1950: the folding full suspension mountainbike. In contrast to the Montegue models, the generation of this top-tech bike was developed entirely in-house. BMW’s experience from the motorbike sector was pumped into the pedal-powered two-wheelers. The front wheel was sprung with the BMW Telelever system, which combined a telescopic fork with a pinion. The advantage of this was that, when braking, the suspension was less involved. The risk of sailing over the handlebars, especially when descending a mountain, was reduced. 

Meanwhile, the bike market had become visibly segmented. Mountainbikes in all manner of variations were as much in demand as trekking bikes and city bikes. BMW responded to these demands with a product range of its own. In the summer of 1999, the Munich firm unveiled the Q6.S mountainbike and the Q5.T Touringbike, the first two models from the Q-Bike series. The frame, complete with folding mechanism, was a patented invention by BMW and the Telelever was enhanced further. Hydraulic disc brakes from Magura and top-quality drive components from Shimano XT and XTR made the mountainbikes the best bikes in their class. In 2002, BMW also entered the racing bike market. Components that could withstand the rigours of racing, a fork made from carbon and an ultra-light aluminium frame were the features of the Q8.R – which was also the only bike in the Q-Bike range (1999-2004) that did not fold.

The new BMW Bike Generation 
Mobility, just as it has always been, is the most important factor for BMW bikes. With the Cruise Bike, the Touringbike, the Enduro and Cross Country Mountainbikes, BMW is now taking standards to another level. The folding mechanism was completely done away with in order to improve the weight and stability of the fourth generation of bikes. The quick-release function of individual components means that easy handling and simple transport are guaranteed, however. The tradition of BMW’s bicycles is therefore still evident in the latest collection. The pleasure of driving is assured with extensive tests, bike trials and strict quality criteria that are enforced just as much with bikes as they are with all of BMW’s other products. 

For queries or information, please contact:
Corporate Communications
Giuseppe Faranna, BMW Group, PR Programme MINI und BMW
Telefon: +49-89-382-51735, Fax: +49-89-382-28017
Michael Kirsch, BMW Group, Leiter Public Relations
Telefon: +49-89-382-25111, Fax: +49-89-382-28017
Internet: www.press.bmwgroup.com
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Sporty driving machine on two wheels.

The BMW Mountainbike Cross Country.
Munich. No up-hill road is too steep, no down-hill cruise too slow nor any race too tough anymore – the BMW Mountainbike Cross Country is the roadster in its category. Whatever route you decide to take, you will experience it with all the intensity a fully has to offer. 
Equipped with the very latest in technology, such as the “Stable Platform Valve” from Manitou and the sophisticated four-jointed rear construction, the tour on a BMW Cross Country Bike will become a special but safe kind of experience. The Manitou R 7Super sprung fork also has a lock-out function and the blockade can be disengaged at any time – even while cycling – via a remote lever on the handlebars. The rebound damping on the shock absorber and sprung fork can be adjusted individually. The travel is 100 mm.

The changer and gear lever from the X.0 series by SRAM are used in professional competitions and are the first choice for demanding racers when it comes to optimum and easy drive. The derailleur Simano XTR, the pedals Shimano PD-M 540 and crank bearing FSA Carbon Issue Team together with the fully-hydraulic disc brakes from Magura with a weight of just under 350 grams guarantee a high riding quality. 
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The central element is the silver aluminium frame with a hydroformed upper bar. It reflects the unique BMW design – similar to the design lines of the car – with concave and convex surfaces. The aesthetic fork and the compensator anodized with copper, together with the BMW logo in a 3D design, complete the appearance of the bike, making it a real eye-catcher. The bike weighs just 11.6 kg. 

The Mavic Crossmax wheels have a special additional feature: They are suitable for the use of tubeless tyres. Two further details: The BMW Mountainbike Cross Country can be transported in all BMW carrier systems. And to ensure that the race doesn’t become too much like thirsty work, a bottle holder is provided on the lower bar.
The new generation of BMW Bikes

Since 1946, BMW has had experience in building bikes, and has operated its own product line since 1992. Just as in the past, BMW has developed and designed its bikes exclusively in-house. 

The BMW Cruise Bike is available in frame sizes S, M and L, the Touringbike in S, M, L and XL, the Mountainbike Enduro in M and L and the Mountainbike Cross Country is available in frame sizes M, L and for the first time also in XL. As of now, the BMW Bikes will be available from selected BMW dealers. 
The price of the BMW Mountainbike Cross Country is Euro 4,199 (price in Germany). More information can also be found online at www.bmw-shops.com. 

Fine-grade photographic material can be downloaded from the BMW Group PressClub at www.press.bmwgroup.com.
For queries or information, please contact:
Corporate Communications
Giuseppe Faranna, BMW Group, PR Programme MINI und BMW

Telefon: +49-89-382-51735, Fax: +49-89-382-28017

Michael Kirsch, BMW Group, Leiter Public Relations

Telefon: +49-89-382-25111, Fax: +49-89-382-28017
Internet: www.press.bmwgroup.com

e-mail: presse@bmw.de
The BMW Mountainbike Cross Country 2007 at a glance:
Colour: Silver 

	Frame
	Aluminium full suspension, BMW design with integrated BMW logo, monochrome silver, copper compensator 

	Fork
	Manitou telescopic air fork R-7 Super Click Remote Lockout, 100 mm, suspension travel

	Dampers
	Air suspension element Manitou S-Type with SPV platform, adjustable rebound phase damping, 100 mm suspension travel

	Handlebars
	Ritchey WCS MTB handle bar, matt black

	Stem
	Ritchey WCS

	Cranks 
	FSA Carbon Team Issue, length 175 mm, 44/32/22 tooth

	Brakes
	Magura Marta hydraulic disc brakes, 180/160 mm

	Wheel set
	Mavic Crossmax ST (suitable for tubeless tyres)

	Tyres
	Continental Explorer Supersonic, 26x2.10, black, foldable

	Drive train
	SRAM X.0, 27-speed, grip shift gears

	Rear derailleur
	SRAM X.O longcage 

	Front derailleur
	Shimano XTR Topswing 

	Shifter
	SRAM X.O grip shift

	Cassette
	SRAM PG–990 11-32 teeth

	Chain
	Shimano XTR CN-7701

	Saddle
	Fi’Zi:k Gobi titan black 

	Saddle stem
	Ritchey WCS, length 350 mm, D=31.6 mm, matt black 

	Pedals
	Shimano PD-M 540

	Weight
	11.6 kg

	Frame height
	M (47 cm), L (52 cm), XL (55cm) 
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For demanding bikers. 

The BMW Enduro Special Edition mountain bike.
Munich. More possibilities, more speed, more adrenaline – BMW already set the standards last year with the Enduro mountain bike. The new Special Edition adds yet another dimension to all-terrain biking: equipped with the finest components, it offers demanding bikers unlimited passion. 

Perfection down to the last detail

Alongside the finish and the design, the focus in the special edition of the BMW Enduro mountain bike lies on its components. The bike’s entire drive train is made up of the new XTR series from market leader Shimano. The Special Edition is the first BMW bike to come equipped with components from this XTR series. From the SL-M970 gear lever, a new development from Shimano for even faster, uncompromising gear changing, through to the FC-M970 crankset, all of the bike’s components are perfectly coordinated with each other: From the brake, the high-end gear and brake levers and tripartite sprocket cassette right through to the newly-developed crankset. 

The Special Edition’s front wheel suspension is taken care of by the Manitou Nixon Platinum Intrinsic sprung fork. The bike’s most eye-catching feature is its aluminium frame in Phoenix Yellow, made using the deep-drawing method, complete with concave and convex surfaces.  

The new generation of BMW Bikes

Since 1946, BMW has had experience in building bikes, and has operated its own production line since 1992. Just as in the past, BMW has developed and designed its bikes exclusively in-house. 

The BMW Cruise Bike is available in frame sizes S, M and L, the Touringbike in S, M, L and XL, the Mountainbike Enduro in M and L and the Mountainbike Cross Country is available in frame sizes M, L and for the first time also in XL. As of now, the BMW Bikes will be available from selected BMW dealers. 

The BMW Enduro Special Edition mountain bike costs Euro 4,499 in Germany and will be available as of now. More information can also be found online at www.bmw-shops.com. 

High resolution photographic material can be downloaded from the BMW Group PressClub at www.press.bmwgroup.com.

For queries or information, please contact:
Corporate Communication

Giuseppe Faranna, BMW Group, PR Programme MINI und BMW

Telefon: +49-89-382-51735, Fax: +49-89-382-28017

Michael Kirsch, BMW Group, Leiter Public Relations

Telefon: +49-89-382-25111, Fax: +49-89-382-28017
Internet: www.press.bmwgroup.com

e-mail: presse@bmw.de
The BMW Enduro Special Edition mountain bike 2007 at a glance:

Colour: Phoenix Yellow
	Frame
	Fully-sprung aluminium with four-jointed rear construction, BMW design with integrated BMW logo, twin-colour Phoenix Yellow and shiny black

	Fork
	Air-sprung Manitou telescopic fork, Platinum Intrinsic ITTravel adjust aluminium shaft with variable travel adjustment from 35 to 145 mm

	Shock absorbers
	Manitou Swinger X3 190/50 with SPV platform, travel 145 mm

	Handlebars
	MTB Lowriser X-TAS-Y AL 2014DB handlebars in matt black

	Stem
	BMW original MTB in matt black (adjustable incline) including BMW logo

	Crankset
	Shimano KRG XTR FC-M970 with bearings without cooling lubricant 175 mm, crank length 44/32/22 tooth 

	Brakes
	Shimano XTR 180/160

	Wheel set
	Mavic Crossmax ST

	Tyres
	Continental Gravity Pro  57-559 black, folding

	Drive
	Shimano XTR, 27 gear derailleur, Rapid Fire including gear lever

	Gears
	Shimano XTR RD-M 970SGS

	Derailleur
	Shimano XTR E-Type

	Gear lever
	Shimano XTR SL-M970 

	Sprocket cassette
	Shimano XTR CS-M970 11-34

	Chain
	Shimano XTR CN-7701

	Saddle
	Fi’Zi:k Gobi Titanium   black

	Saddle support
	Ritchey WCS V2 length 350mm, D=31.6 mm, matt black

	Pedals
	Shimano PD-M 540

	Weight
	13.5 kg 

	Frame height
	M (45 cm), L (50 cm)
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Unbridled passion.

The BMW Mountainbike Enduro.
Munich. More options, more pace, more adrenaline – the new BMW Mountainbike Enduro offers all possibilities to really sophisticated bikers. No matter whether it is free ride, you ride an easy slope or challenge the Tremalzo Pass. The design of the BMW Mountainbike Enduro alone, with its concave and convex surfaces, also reflects the pure energy of motion. A fully suspension bike which delivers sheer driving pleasure at a high degree.
Exceptional details for discerning riders

BMW’s dedication to excellence in the manufacture of its products and use of only the best materials applies to its bike designs too. Experience from the field of automobile construction is woven into the stable aluminium frame, which has been manufactured using the deep-drawing method. This technology makes special design features possible, similar to the lines of the automobile, with concave and convex surfaces. The discreet BMW logo and the twin-colour powder coating in matt gold and matt black highlight the design once again.  

The sprung fork and rear suspension boast contrasting colours, but have the same top-quality technology as the frame. The four-jointed rear construction delivers sensitive contact behaviour without any drive influences through the Platform Plus technology by Manitou. The Manitou Radium air cushion, with 145 mm travel in sizes M and L, provides the ideal suspension solution. At the front, the air-sprung, Manitou Minute air-telescopic suspension fork absorbs the harshest shocks with 140 mm travel. 
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State-of-the-art technology helps take cyclists to the top: the Platform Plus function of the rear wheel suspension suppresses severe see-sawing of the bike when the cyclist steps on the pedals. The shock-absorber also comes equipped with a “lock-out” lever, which closes the pressure stage and turns the bike into a hard-tail without see-saw effects. If the cyclist ever forgets to release the blockade in rough terrain, an overpressure valve protects the absorber from damage. The sprung fork boasts Infinite Travel Adjust (IT) technology. At the press of a button, it steplessly reduces the travel of the fork from 140 to a minimum of 35 millimetres, thereby adapting the geometry of the bike perfectly to the incline. Consequently, rapid changes between climbs and descents are no longer a problem. The remote control on the handlebars means that the travel can even be adjusted for the fork while on the move.

To ensure that a downhill trip doesn’t turn into a descent into hell, the BMW Mountainbike Enduro has hydraulic disc brakes at the front and rear. With the hydraulic brake Hayes Nine, the right speed is just a good pull on the hydraulic lever away – no matter what the weather. So when things need to be notched up a gear, the components of the X.9 gear system from SRAM deliver the necessary drive. The 27 gears can be selected easily and precisely with the X.9 trigger levers.

Accessories

The BMW bike offers many options as far as accessories are concerned : There are fastenings for the bottle, and the right tool – a must for every trip – can be obtained from BMW’s accessories range. And what if the final destination is the car park? With the BMW Mountainbike Enduro, which weighs just 14.5 kilograms, the trip continues without any problems: in the BMW’s roof carrier system.

The new generation of BMW Bikes

Since 1946, BMW has had experience in building bikes, and has operated its own production line since 1992. Just as in the past, BMW develops and designs its bikes exclusively in-house. 
The Cruise Bike is available in frame sizes S, M and L, the Touringbike in S, M, L and XL, Mountainbike Enduro in M and L and the Mountainbike Cross Country is available in frame sizes M, L an for the first time also XL. As of now, the BMW Bikes will be available from selected BMW dealers. 

The price of the BMW Mountainbike Enduro is Euro 2,699 (price in Germany). More information can also be found online at www.bmw-shops.com. 

Fine-grade photographic material can be downloaded from the BMW Group PressClub at www.press.bmwgroup.com.

For queries or information, please contact:

Corporate Communications 

Giuseppe Faranna, BMW Group, PR Programme MINI und BMW

Telefon: +49-89-382-51735, Fax: +49-89-382-28017

Michael Kirsch, BMW Group, Leiter Public Relations

Telefon: +49-89-382-25111, Fax: +49-89-382-28017
Internet: www.press.bmwgroup.com

e-mail: presse@bmw.de
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The BMW Mountainbike Enduro 2007 at a glance:
Colour: Matt Gold 
	Frame
	Full aluminium suspension with four-bar rear end, BMW design with integrated BMW logo, two-colour in matt gold and matt black

	Fork
	Telescopic air fork Manitou Minute Platinum Air IT Travel Adjust aluminium stanchion with variable suspension travel setting 35 – 140 mm

	Dampers
	Manitou Radium RL-Air with lock-out function, length 190 mm, suspension travel 145 mm 

	Handlebar
	Humpert MTB lowriser handlebar, aluminium 610 mm, matt black

	Stem
	BMW original MTB matt black (with adjustable angle) including BMW logo

	Cranks
	Truvativ KRG Firex Team Giga X Pipe 44/32/22 tooth, length 175 mm metal grey front sprocket

	Brakes
	Hayes HFX-Nine V7/V6 disc brakes, hydraulic, 180/160 mm rotor

	Wheel set
	DT-Swiss wheels EX-5.1 D, hub set DT-Swiss Onyx Disc black, spoke DT-Swiss Competition 2.0/1.8/2.0, DT-Swiss quick-release set

	Tyres
	Continental Gravity Pro, folding, 26 x 2.3

	Drive train
	SRAM X.9, 27-speed chain gear, trigger shifter

	Rear derailleur
	SRAM X.9 silver

	Front derailleur
	Shimano Hone, E-Type

	Shifter
	SRAM X.9, trigger

	Cassette
	SRAM PG970 11-34-tooth

	Chain
	SRAM PC971

	Saddle
	Fi’Zi:k Nisene Sport, black

	Saddle support
	Kalloy, length 350 mm, D=31.6 mm, matt black

	Pedals
	Wellgo Dual pedals with click system

	Weight
	14.5 kilograms

	Frame height
	M (45 cm); L (50 cm)
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Take a seat and feel good. 

The BMW Cruise Bike.
Munich. Busy avenue or empty boardwalk at the beach: The BMW Cruise Bike invites you to enjoy life on a two-wheeler. Especially striking attributes are its individuality, the distinctive design and the dynamics. Exploring the city has never been such a pleasurable experience.
California is the traditional home of Cruise Bikes, and from Munich comes a new interpretation of the Cruiser. A trip to the beach or into town? It doesn’t really matter, as long as you stay relaxed. And the frame’s state-of-the-art geometry takes care of that, ensuring optimum seating comfort. The innovative hydroforming technology gives the frame its unique design and shape. Lines similar to the automobile and a discreetly integrated BMW logo leave no doubt about the bike’s origins. 

Equipped with a 24-gear Alivio control unit from Shimano, the bike is equally at home around lakes or in the mountains. Even cruising in hilly environments becomes a pleasure. The BMW Cruisebike’s unassailable advantage lies in its versatility. It looks equally good on a beach promenade as on a forest path: the Suntour NRX-6000 telescopic suspension fork effortlessly counteracts uneven terrain. And there’s no need to worry about sufficient braking power as the Cruiser’s Shimano V brakes stop the bike quickly; the brake cables for the rear brake are integrated within the frame.
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Wheel guard covers and other standard cycle parts can be quickly fitted as accessories. Moreover, the Cruiser’s frame, which is available in the colours pearl white and champagne, is suitable for usual child seat models with standard frame assembly. The Cruiser’s frame takes popular market models of child seats with standard frame assembly. And if it’s a little distance to the start of the next tour, the bike can easily be transported in the BMW rack system. In addition to that, the standard side stand guarantees safe parking during breaks or at the end of your tour. 

The new generation of BMW Bikes

Since 1946, BMW has had experience in building bikes, and has operated its own production line since 1992. Just as in the past, BMW has developed and designed its bikes exclusively in-house. 
The BMW Cruise Bike is available in frame sizes S, M and L, the Touringbike in S, M, L and XL, the Mountainbike Enduro in M and L and the Mountainbike Cross Country is available in frame sizes M, L and for the first time also in XL. As of now, the BMW Bikes will be available from selected BMW dealers. 

For its unique combination of high-quality design and outstanding safety details, the BMW Cruise Bike was awarded the renowned iF product design award 2006 and the reddot design award 2006.
The price of the BMW Cruise Bike is around Euro 829 (price in Germany). More information can also be found online at www.bmw-shops.com. 

Fine-grade photographic material can be downloaded from the BMW Group PressClub at www.press.bmwgroup.com.

For queries or information, please contact:
Corporate Communications

Giuseppe Faranna, BMW Group, PR Programme MINI und BMW

Telefon: +49-89-382-51735, Fax: +49-89-382-28017

Michael Kirsch, BMW Group, Leiter Public Relations

Telefon: +49-89-382-25111, Fax: +49-89-382-28017
Internet: www.press.bmwgroup.com

e-mail: presse@bmw.de
The BMW Cruise Bike 2007 at a glance:
Colour 1: Pearl White 

	Frame
	Aluminium front suspension, BMW design with integrated BMW logo, monochrome, pearl white

	Fork
	Suntour NRX-6000, telescopic fork, 75mm travel, integrated mudguard mounting

	Handlebar
	City Cruiser 23º, 605mm, matt black

	Stem
	BMW original MTB matt black, (angle-adjustable) including BMW logo

	Cranks
	Shimano Alivio FC-M411, 42/32/22 teeth, length 170 mm with chain guard disc

	Brakes
	Shimano Alivio V-Brake, BR-M421-S, black

	Hubs
	Shimano VR + HR  / 32 hole, with quick-release set, black

	Rims
	Rodi Airline Plus, 19-559 eyelets, 32 hole system, polished sidewalls, black

	Tyres
	Continental City Contact with reflective stripes, 26x2.10

	Drive train
	Shimano Alivio, 24-gear derailleur, Rapid Fire shift lever

	Rear derailleur
	Shimano Alivio RD-MC410, black

	Front derailleur
	Shimano Alivio FD-M410 

	Shifter/ brake lever
	Shimano Alivio ST-M410, black 

	Cassette
	Shimano CS–HG30, 11-32 tooth

	Chain
	Shimano CN–HG40

	Saddle
	Selle Royal Freccia

	Saddle stem
	Kalloy, length 350 mm, D=27.2 mm, black

	Pedals
	Sports pedals with reflectors

	Weight
	14.1 kg 

	Frame height
	S (41 cm); M (46 cm); L (51 cm)

	Road equipment
	Bell, stand and reflectors (included) 


The BMW Cruise Bike 2007 at a glance:
Colour 2: Champagne

	Frame
	Aluminium front suspension, BMW design with integrated BMW logo, monochrome, champagne 

	Fork
	Suntour NRX-6000, telescopic fork, 75mm travel, integrated mudguard mounting

	Handlebar
	City Cruiser 23º, 605mm, matt black

	Stem
	BMW original MTB matt black, (angle-adjustable) including BMW logo

	Cranks
	Shimano Alivio FC-M411, 42/32/22 teeth, length 170 mm with chain guard disc

	Brakes
	Shimano Alivio V-Brake, BR-M421-S, silver

	Hubs
	Shimano VR + HR  / 32 hole, with quick-release set, silver

	Rims
	Rodi Airline Plus, 19-559 eyelets, 32 hole system, polished sidewalls, silver

	Tyres
	Continental City Contact with reflective stripes, 26x2.10

	Drive train
	Shimano Alivio, 24-gear derailleur, Rapid Fire shift lever

	Rear derailleur
	Shimano Alivio RD-MC410, silver

	Front derailleur
	Shimano Alivio FD-M410 

	Shifter/ brake lever
	Shimano Alivio ST-M410, silver

	Cassette
	Shimano CS–HG30, 11-32 tooth

	Chain
	Shimano CN–HG40

	Saddle
	Selle Royal Freccia

	Saddle stem
	Kalloy, length 350 mm, D=27.2 mm, black

	Pedals
	Sports pedals with reflectors

	Weight
	14.1 kg 

	Frame height
	S (41 cm); M (46 cm); L (51 cm)

	Road equipment
	Bell, stand and reflectors (included) 
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Superb in the saddle.

The BMW Touringbike.
Munich. Green meadows, dark soil, colourful woods – with the BMW Touringbike every tour will be unique. It is not only a motorists’ privilege to have quality, comfort and sophisticated technology at the highest level and the BMW Touring Bike meets all these requirements – from the front wheel to the rear reflector.
How about a bike ride at the weekend? With the BMW Touringbike, that’s not a problem. Slopes both big and small are quickly overcome thanks to the 27-gear derailleur. The Deore control unit from Shimano makes changing gears as easy as ringing the bell. Just one touch of the Rapid Fire gear lever is all it takes to make the trip last longer. The gel saddle and sprung saddle supports guarantee cycling enjoyment that lasts for miles. And to ensure that the trip doesn’t have to end prematurely at the city limits, the Touringbike comes with everything it needs to comply with road traffic licensing regulations. From the wheel protector and light sensor to the parking light function and reflector, everything needed to make cycling safer and comply with road traffic licensing regulations is there. 

Even in the hippest parts of town, you can sit easy in the saddle. The bike’s unusual design makes it a real eye-catcher. The innovative hydroforming technology transfers the classical lines of the automobile to the design of the cycle frame that has the colour light grey. The integrated BMW logo creates the perfect look.

On the road home, cobblestones and kerbstones stand no chance of spoiling the pleasure. The 75-mm travel of the Suntour NRX 6500 telescopic suspension fork made of magnesium, with lock-out function, counteracts unevenness and makes even the next cycling trip along unsecured path a pleasure. 

The HS11 hydraulic rim brakes from Magura perform reliably and with exceptional deceleration values. The brake cables are integrated into the inside of the frame, as is the rear light cable. Once the prop stand has been folded out, the Touringbike is ready for its next trip. Maybe with some provisions in the saddle bags, or a picnic basket? There’s plenty of room on the luggage carrier with an integrated air pump, in case you need to help someone out with a flat tyre en route. The Touringbike is also perfectly equipped for longer trips. On the car roof, in the BMW carrier system, it cuts a fine figure until the next time it’s used. 

The new generation of BMW Bikes

Since 1946, BMW has had experience in building bikes, and has operated its own production line since 1992. Just as in the past, BMW has developed and designed its bikes exclusively in-house. 
The BMW Cruise Bike is available in frame sizes S, M and L, the Touringbike in S, M, L and XL, the Mountainbike Enduro in M and L and the Mountainbike Cross Country is available in frame sizes M, L and for the first time also in XL. As of now, the BMW Bikes will be available from selected BMW dealers. 
The price of the BMW Touringbike is Euro 1,239 (price in Germany). More information can also be found online at www.bmw-shops.com. 

Fine-grade photographic material can be downloaded from the BMW Group PressClub at www.press.bmwgroup.com.

For queries or information, please contact:
Corporate Communications

Giuseppe Faranna, BMW Group, PR Programme MINI und BMW

Telefon: +49-89-382-51735, Fax: +49-89-382-28017

Michael Kirsch, BMW Group, Leiter Public Relations

Telefon: +49-89-382-25111, Fax: +49-89-382-28017
Internet: www.press.bmwgroup.com

e-mail: presse@bmw.de
The BMW Touringbike 2007 at a glance:
Colour: Light Grey

	Frame
	Aluminium, front-sprung, BMW design with integrated BMW logo, one-colour (powder-coated), light grey

	Fork
	Telescopic fork Suntour NRX 6500 Magnesium with aluminium stanchion, 75 mm suspension travel with lock-out function, integrated mudguard mounting, shiny black

	Handlebar
	MTB lowriser handlebars, aluminium 580 mm, matt black 

	Stem
	BMW original MTB matt black (with adjustable angle) including BMW logo, matt black 

	Cranks
	Shimano FC–M540 48/36/26-tooth Hollowtech, length 170 mm with chain guard disc, silver

	Brakes
	Magura HS11 hydraulic rim brakes with Evo Adapter 

	Hubs
	Shimano VR hub dynamo DH-3N30 silver QR type , FH-M530 Deore QR type / 32-hole, silver

	Rims
	Rodi Airline Plus, 19-559 eyelets, polished sidewalls, silver, 32 hole system

	Tyres
	Continental Contact with reflective strips, 26 x 1.75

	Drive train
	Shimano Deore, 27-speed chain gear, Rapid Fire

	Rear derailleur
	Shimano Deore RD-M511-s silver Top Normal

	Derailleur
	Shimano Deore FD-M531

	Shifter
	Shimano Deore SL-M511, 27 gear

	Cassette
	Shimano CS-HG50/9 11-34 tooth

	Chain
	Shimano CN-HG53

	Saddle
	Selle Royal Athletic Look-in, 3-layer gel construction, black, 2317 DG Xenium cover with side protection

	Saddle stem
	Kalloy with suspension, SP-380, length 300 mm, D=27.2 mm, matt black

	Road equipment
	Mudguards in special colour matt grey, lighting with sensor lamp, rear light with sidelight function, stand, pump, bell

	Luggage rack
	Pletscher Mercury, black with attachment

	Chain guard
	De Woerd Chain Cap Transparent for 48 teeth

	Pedals
	Aluminium with reflectors

	Weight
	17.1 kg 

	Frame height
	S (41 cm); M (46 cm); L (51 cm); XL (55 cm)
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Exciting ride for little cyclists. 

The new BMW Cruise Bike Junior.  
Munich. For young cyclists who want to go far, the new Cruise Bike Junior from BMW will be available as of March 2007. The bike in a 20” size, especially tailored to children aged between 5 and 8, inspires the up-and-coming cyclists with dynamic riding fun and a cool look in an unmistakeable BMW design. However, the BMW Cruise Bike Junior is not only popular with the kids: parents are also happy with the resilient, maintenance-free equipment, the sturdy technology and the high-quality safety features.  

Fledgling cyclists from around two and a half years of age can experience the enjoyment of cycling for the first time with the BMW Kidsbike, which can be converted from a learner bike to a child’s bike. However, at some point, even the little ones become too big for it. This is where the new BMW Cruise Bike Junior comes into its own. With its wheel size of 20”, it is the ideal playtime companion for older kids. The geometry of the high-strength aluminium frame is perfectly tailored to the build of a child. Thanks to the high-performance hub gear, the little cycling fans can overcome any hill with ease.  

The older children get, the more they come into contact with road traffic. Safety is therefore top priority with the BMW Cruise Bike Junior. Three independent brakes – 2 calliper brakes, 1 back pedal brake – enable a short braking path. The grip width of the child-orientated brake lever can be adjusted to any child’s hand size. Optimum visibility at any time of day or year is guaranteed by the reflectors, safety pedals with light diodes and reflective strips on the wide balloon tyres. 

No driving licence yet and already driving a BMW: the BMW Cruise Bike Junior is entirely modelled along the lines of its “grown-up” siblings and makes a tremendous impression with its dynamic forms and proportions in the typical BMW design. A 3D version of the BMW logo also decorates the frame. 

Additionally, the entire bike, including all components, bears a DIN Plus test certificate. The features of the bike include a 3 gear hub, a suspension fork with 50 mm travel as well as gear cable and brake cable guides, which are integrated into the frame. The standard equipment also includes the sturdy side stand. 

As of now, the BMW Cruise Bike Junior will be available for boys and girls from selected BMW dealers and on the Internet at www.bmw-shops.com.

High resolution photographic material can be downloaded from the BMW Group PressClub at www.press.bmwgroup.com.

For queries or information, please contact:
Corporate Communications

Giuseppe Faranna, BMW Group, PR Programme MINI und BMW

Telefon: +49-89-382-51735, Fax: +49-89-382-28017

Michael Kirsch, BMW Group, Leiter Public Relations

Telefon: +49-89-382-25111, Fax: +49-89-382-28017
Internet: www.press.bmwgroup.com

e-mail: presse@bmw.de
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Sheer Riding Pleasure. From the very beginning.

The BMW Kidsbike enables children to enjoy a bicycle without stabilisers.
Munich. With the multiple award-winning BMW Kidsbike, children experience from the very beginning what it feels like to discover the world on two wheels – and entirely without stabilisers. The key here is that the bike grows with the child! For the little ones from about age two and a half, it is a walking bike. Later the child can use pedals: simply mounting the supplied pedal unit turns the BMW Kidsbike into a full-fledged children’s bicycle, allowing 6-year-olds to experience sheer riding pleasure too.

Using the walking bike, the little ones can naturally train their sense of balance and gain some initial experience of setting off, steering and braking. As soon as a child feels safe enough, the BMW Kidsbike enables a seamless and child-oriented transition to real cycling on the same bike: the pedals and chain unit are mounted in a few simple steps.

The dynamic proportions of the new Kidsbike demonstrate that you are never too young for a real BMW, with convex and concave surfaces in the characteristic BMW design. “Form follows function”: the saddle design persuades bikers with improved ergonomics. The innovative frame in highly rigid aluminium consists of a single countersunk and curved multichamber extrusion profile which has a number of surprisingly practical functions such as an integrated bag. Specially designed components such as the functional impact protection complete the distinctive appearance of the new BMW Kidsbike 2006. 

If things do get a bit rough now and again from sheer riding pleasure, the BMW Kidsbike provides optimum safety. The adjustable cantilever front wheel brake is particularly easy to operate. The mounted pedals also have a back pedal brake which ensures a short braking distance. An important point at dusk: the 

integrated synthetic pedals are fitted with reflectors, and reflective strips on the 14” tyres provide an enhanced signalling effect at night. A bell and the passive lighting are part of the standard equipment as well as the children’s bike helmet with TÜV/GS and EN 1071 certification. Further safety features of the BMW Kidsbike include a child-oriented handlebar design, a fully encapsulated chain, a limited steering stop limit and a protective pad on the handlebars (with additional storage compartment) and an upper tube.

The permitted maximum load of the 6 kg BMW Kidsbike (8 kg with pedals) is around 50 kg. Seat height is variably adjustable between 38 and 46 centimetres.

The BMW Kidsbike was awarded the EUROBIKE AWARD 2005 for its unique combination of high-quality design and outstanding safety details. It also won the renowned iF product design award 2006, as well as the reddot design award 2006.

The BMW Kidsbike in orange and blue including accessories is available for 259 euros (recommended retail price for Germany) from selected BMW partners and online at: www.bmw-shops.com. And if this bike gets too small, there will be the new BMW Cruise Bike Junior available as of now for children from age 5. 

Photos in fine data quality are available in the BMW Group PressClub at www.press.bmwgroup.com.

For queries or information, please contact:  
Corporate Communications

Giuseppe Faranna, BMW Group, PR Programme MINI und BMW

Telefon: +49-89-382-51735, Fax: +49-89-382-28017

Michael Kirsch, BMW Group, Leiter Public Relations

Telefon: +49-89-382-25111, Fax: +49-89-382-28017
Internet: www.press.bmwgroup.com

e-mail: presse@bmw.de
PAGE  

