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•
High-quality entertainment systems, optionally with multichannel 
audio, USB audio connection, iPhone and iPod integration. 

•
Four-zone automatic air conditioning and Active Seat 
Ventilation as optional extras.

•
Additional safety provided by Rear View Camera and Side View.
With its extensive and innovative range of equipment, the BMW X6 stands 
as a symbol of significant progress in the field of vehicle travel comfort. 
Even with its standard range of equipment, the Sports Activity Coupé fulfils the highest demands of premium quality. For example, standard equipment includes the high-quality entertainment system with MP3-capable CD drive and AUX-IN socket, automatic air conditioning, Electromechanical Parking Brake, cruise control with brake function and Park Distance Control at the rear of the vehicle. The likewise standard shift paddles at the steering wheel and 
the multifunction steering wheel further enhance the sporty driving experience offered by the BMW X6. Other individual comfort requirements can be fulfilled with a varied range of attractive and innovative special equipment features and accessory options, some of which are exclusive to BMW. Highlights include 
the individually adjustable electrical open and close mechanism for the tailgate, Active Seat Ventilation and the automatic Soft Close system for the doors. 
With the likewise optionally available Rear View Camera and the Side View system – available as an accessory – both travel comfort and safety are further enhanced in the BMW X6.

In the BMW X6, the control of the air conditioning and entertainment system 
is as standard via the operating system iDrive – which can optionally be 
used for navigation and communication, too. The settings are made intuitively by turning, pushing and pressing the iDrive Controller in the central console, with selected functions and adjustment options shown in the Control Display. In order to optimise the functional efficiency of iDrive, there are eight individually assignable favourite buttons. In this way, a single press of a 
button allows a frequently called telephone number, a regularly selected travel destination or a preferred radio station to be accessed instantly. 

High-quality on-board entertainment: no journey is too long.

Time is a rare asset and yet there is a niche in which it is possible to create 
a sense of timelesseness: in a motor vehicle. The BMW X6 offers the very best conditions for leisure and enjoyment. All CD players available for the BMW X6 are also able to play music in MP3 format. Thanks to the AUX-IN socket which comes as standard, or the optionally available USB interface, music can 
also be played from external audio sources such as MP3 players, with excellent audio quality provided by the vehicle loudspeakers. The directory and 
file structure of the external medium – be it an Apple iPod or a USB stick – automatically appears in the iDrive display and can be operated via the 
on-board operating system. Another bonus: individual titles can be selected using the iDrive favourite buttons.

Incomparable surround sound: multichannel audio system.

Even with standard equipment, the six high-quality speakers of the 
Radio Professional system provide an impressive audio experience. Two central bass speakers are located underneath the front seats, the mid-range 
speakers are fitted in the four door panels. 

The optionally available HiFi speaker system with 12 loudspeakers and the likewise optional HiFi System Professional with 16 speakers offer digital equalizing, which enables the sound quality to be adjusted individually for each seat. In conjunction with the optional 6-DVD changer, the HiFi System Professional is able to play multichannel audio formats for even more intense audio pleasure. The multichannel audio system creates a fascinating sound which is especially effective in bringing out sophisticated sound effects. 
The interference-free acoustic pressure was also doubled in this system as compared to the HiFi speaker system. 

Navigation system and mobile phone interface.

A particular comfort highlight which is optionally available for the BMW X6 
is the navigation system Professional. Its features include a high-resolution, 
8.8 inch graphic Control Display. One element of the navigation system Professional is a new and highly reliable voice control system which is exclusively available for BMW vehicles. It enables whole-word voice entry 
of a destination, making for time-saving convenience when entering 
a destination.

Thanks to the additionally available mobile phone preparation with 
Bluetooth interface, numerous mobile phones with Bluetooth capacity which are commonly available on the market – including the Apple iPhone – can 
be networked with the electronic system of the BMW X6. This enables mobile phones to be operated conveniently and safely inside the vehicle using 
the hands-free facility and the multifunction buttons on the steering wheel. 
The address book, call lists and other data are automatically synchronised 


with the on-board system. A snap-in adaptor connects the mobile phone to the vehicle aerial, charging it at the same time. The integration of the Apple iPhone enables fully integrated operation of the telephone or entertainment function 
of the device using the iDrive operating system.

Innovative DVD system at the rear.

For the central console at the rear a DVD video system is optionally available, also with TV reception if desired. The 8-inch TFT colour monitor is simply folded down flat into central console if space is required for transporting larger items. The DVD player integrated in the rear console can play audio, video 
and photo DVDs or CDs. An AUX-IN socket is provided so that external video sources can be hooked up such as game consoles or video cameras.

Differences of opinion among child passengers can be avoided with 
the innovative DVD System Advanced, taken from the range of Original BMW Accessories. It encompasses two 7-inch monitors which are mounted on 
the seatbacks of the front seats, and there is no contact between these and the headrests. The two screens in authentic 16:9 cinema format can thus be individually adapted to the viewing angle of the vehicle occupant in question. 
A key distinguishing feature here is that the monitors can be used with 
the DVD player or with other external sources.

Exemplary driver support with BMW TeleServices.

No other vehicle manufacturer provides such an extensive customer service 
via networked systems like BMW. With a range of services clustered 
under the name of BMW ConnectedDrive, BMW has occupied a pioneering position in this field for many years, too. In addition to the BMW Online website 
and the telematics service BMW Assist, the driver of the BMW X6 also 
has BMW TeleServices at his disposal. Here, services available range from 
the Automatic Teleservice Call to the Manual Teleservice Call and the 
BMW Teleservice Diagnosis, including Teleservice Assistance. In the case of the Automatic Teleservice Call, the vehicle automatically determines the 
nature and timing of any service required using the on-board diagnosis system known as Condition Based Service (CBS). To co-ordinate a workshop appointment, data relating to the state of the engine oil, brake fluid, brake 
discs and brake liners as well as other wear-and-tear parts can be conveyed to the BMW Service Partner by means of a telephone connection. In the 
case of electronic malfunction, the BMW Teleservice Diagnosis enables the communication of any error codes to BMW Roadside Assistance. If the 
cause of the defect can be eliminated by means of a software reset in the relevant control unit, the command can even be sent directly from the 


BMW Roadside Assistance Headquarters to the vehicle. The requirement for the use of BMW TeleServices is that the vehicle is fitted with a mobile phone preparation with Bluetooth interface.

Park Distance Control (PDC), Rear View Camera and 
Side View function.

With Park Distance Control (PDC), parking becomes a veritable pleasure. Sensors determine the distance of the vehicle from any obstacles, and acoustic signals – whose frequency increases as the distance decreases – indicate 
how much space is left to manoeuvre in. The BMW X6 is fitted as standard with a PDC at the rear, and the system is also optionally available for the front end 
of the vehicle.

As a supplement to PDC, the Rear View Camera is also available for the 
BMW X6. The video system facilitates parking and manoeuvring in spaces which are very limited or difficult to see. The Rear View Camera is 
activated either by pressing a button or automatically when engaging reverse gear, together with PDC. The high-resolution images of the Rear View Camera with wide-angle lens are shown on the Control Display in colour and with optimised perspective. Interactive track lines also indicate the optimum steering wheel angle for parking manoeuvres and the smallest turning 
circle. The video system facilitates parking and manoeuvring in spaces which are extremely tight or offer very poor visibility. It is particularly helpful to use 
the Rear View Camera when hitching a trailer. A zoom function can be used to enlarge the image area so as to focus on the tow hitch. Special static lines 
in the image help estimate the correct distance. An interactive “docking line” relating to the steering wheel angle enables a precise approach to the 
tow bar of the trailer. In frost the camera lens is automatically heated and kept free of ice. 

In addition to the Rear View Camera, the Original BMW Accessories program also includes a Side View function for the new BMW X6. Side View works 
with an additional front end camera which offers a better view of intersecting traffic. In addition to the increased convenience this brings about when manoeuvring, the image relayed to the Control Display provides an early overview of the traffic situation in front of the vehicle – especially when leaving narrow or hidden exits or moving out of multi-storey car parks.

Personal Profile: comprehensive personalisation of vehicle settings.

Be it radio stations, sound settings in the audio systems, preferred temperature adjustments to the air condition system, favourite button settings or seat lighting and Rear View Camera configurations: Personal Profile, a function which comes as standard, ensures the personalisation of numerous vehicle settings. This increases comfort when the BMW X6 is used alternately 
by more than one driver. The data is automatically stored in the remote control 
key when the driver leaves the vehicle and is recalled the next time this key 
is used.

Cruise control with brake function as standard.

The BMW X6 shows premium class in its automatic cruise control, too. 
Unlike conventional systems, the standard cruise control with brake function not only intervenes in engine and transmission management so as to 
maintain a specific speed preset by the driver, it also takes over brake control 
if necessary. A selected speed between 30 km/h and the model-specific maximum can thus be maintained even when the vehicle is travelling downhill and when towing a trailer. The speed is entered by the driver conveniently 
using the steering column control lever and can be set with a high degree of precision in either 1 km/h or 10 km/h stages. 

A wide range of additional functions ensure that the cruise control with 
brake function is able to adapt flexibly to any situation. For example, active brake intervention occurs when the engine drag torque in trailing throttle is not sufficient to maintain the selected speed. On bends, too, the system does not get out of balance thanks to the Curve Speed Limiter (CSL) which electronically incorporates transverse acceleration in the adjustment of the longitudinal acceleration. 

In spite of all this technical support, the driver is always fully in control. The Comfort Dynamic System with its so-called “Manual Throttle Mode” allows manual intervention using the lever at the steering column so as to be 
able to reach the desired speed swiftly or decelerate. This lever or the footbrake can also be used to deactivate the system spontaneously if desired.

Four-zone automatic air conditioning: individualised feelgood 
climate on all seats.

As an alternative to the standard air conditioning, individualised temperature control is also available for the BMW X6. The optional two-zone automatic 
air conditioning enables separate adjustment of the desired temperature and air distribution on both the driver and the front passenger side. With the four-zone automatic air conditioning, this is also possible for the rear, with a separate control element available for rear passengers. There are three climate styles available: “gentle”, “medium” and “intensive”.

Noise-resistant glass slide/tilt roof.

The optional glass slide/tilt roof provides a superb sense of space. 
The electrical operating system for the large-format, interior slide/tilt roof 
can be activated either using a switch inside the vehicle or by means 
of the vehicle key. Its wind-deflecting design reduces the noise level, thus offering additional ride comfort.

An example of a leading, comfort-oriented innovation from BMW is Active Seat Ventilation – a feature which is unique within the entire competitive field. 
This optional fitting for the front seats is available in the BMW X6 in conjunction with comfort seats and seat heating. Active Seat Ventilation ensures enhanced well-being, especially on longer trips. The optimised seat climate also helps alleviate driver fatigue. 

Electromechanical Parking Brake with Automatic Hold as standard.

Driving the BMW X6 – whether through mountain landscapes or in 
stop-and-go traffic – is always a relaxing pleasure. This is ensured by the Electromechanical Parking Brake, a standard feature. With its hydraulically controlled 4-wheel brake intervention function it guarantees outstanding 
brake reliability. With an absolute minimum of operating force, the 
system avoids any inadvertent roll-back on slopes. A particular feature of the Electromechanical Parking Brake is the Automatic Hold function, which automatically keeps the vehicle at a standstill. Not until the driver re-activates the accelerator pedal is the brake function deactivated.

When the drive activates the parking brake switch so as to park the vehicle, 
the mechanical parking brake is set in action by means of an electromechanical system after the engine has been switched off so as to put the BMW X6 
into a secure parking state. In this case, the parking brake only takes effect on 
the rear wheels.

Soft Close system for low-noise door closing.

The Soft Close system for the doors also highlights the outstanding 
comfort standards of the BMW X6. By means of this technology, the doors close automatically, gently and quietly from a pre-lock position of about 
six millimetres. A safety function ensures that doors do not inadvertently fail 
to be closed properly.

As an additional special equipment feature, comfort access allows the vehicle to be opened and started without having to hold the key in one’s hand. As soon as the driver is within 1.5 metres of the vehicle, the vehicle electronic system 

detects the key in the driver’s jacket pocket or bag. Sensors in the exterior door handle then trigger the mechanism for opening or locking the vehicle when 
the driver’s hand touches it. To start the vehicle the driver simply presses the start/stop button while activating the brake pedal. 

Innovative: individually adjustable opening height of the tailgate 
by means of two-stage gas springs.

As an optional extra, the BMW X6 can be fitted with an automatic open 
and close function for the tailgate. At the press of a button and without the application of physical force, the tailgate swings upwards or closes. This standard two-stage gas spring enables the end position of the open tailgate 
to be determined individually, thereby avoiding the risk of damage, 
for example when opening the lid in an indoor car park with a low ceiling. 

In keeping with its large luggage compartment space as compared to competitor models, a wide range of optional extras accessories are available 
for the BMW X6 for the addition of storage facilities. Where the vehicle is 
fitted with the standard runflat tyres, a spare wheel does not need to be carried in the vehicle so there is additional storage space under the luggage compartment floor, which is lockable as standard. This can hold the foldable luggage compartment cover, for example. The optional storage package comprises two lashing bars with four adjustable lashing eyes, storage nets, 
bag hooks, a lighting unit for the storage compartment and a 12 volt socket in the central console. 

The accessory program comprises a luggage net, a luggage compartment fixing strap and a tension belt for securing transport items safely. The luggage net is fixed in front of the load sill and enables smaller load items to be placed so that they are easily at hand. It also ensures that luggage items do not fall 
out of the vehicle when the tailgate is opened. Other perfectly fitting 
Original BMW Accessory items available here are a luggage compartment tub, a water-repellent load space protective cover and a non-slip reversible mat 
for the luggage compartment.

Easy travel with the ski/snowboard holder.

The dynamic BMW X6 cuts a great figure in winter sports areas, too. A rear carrier enables the secure transport of up to four pairs of skis or up to two snowboards. The specially developed ski/snowboard holder is easy to use and harmonises perfectly with the visual design of the vehicle.

In order to the open the tailgate, the rear carrier is simply pushed back, 
even when fully loaded. Special screws and locks provide secure protection from theft. 

Trailer hitch with removable tow ball for loads of up to 3.5 tons.

The Sports Activity Coupé also provides maximum safety when towing a 
trailer. The trailer stability control function comes into operation in conjunction with the optional tow hitch. This system is integrated in the Dynamic Stability Control and is activated as soon as a trailer is connected to the vehicle electronic system via the socket at the rear of the vehicle. On practical feature: the tow ball of the trailer hitch is removable. The trailer facility can support 
a weight of 2.7 tons, or 3.5 tons in the extended special equipment version. 
For the BMW X6 xDrive50i only the 3.5-ton tow option is available.

Intensified wheel orientation with 21-inch light alloy wheels.

In visual terms, the BMW X6 makes a clear statement regarding driving dynamics and supremacy due to its wheel orientation, and as standard the vehicle comes with 19-inch light alloy wheels. To further highlight this 
aspect, there are also wheels available as an optional extra in 20-inch format 
or else 21-inch light alloy wheels from the accessory range in five different variations. All 19 and 20-inch rims have tyres with runflat properties.



•
BMW Spartanburg plant produces the BMW X6 for the 
world market.

•
Expansion into a centre of expertise for BMW X models.

•
Production to BMW standards at the customary high level 
of quality.
Like the BMW X5, the new BMW X6 is produced in its most important 
sales market, the USA, at the BMW Spartanburg Plant in South Carolina. 
Using state-of-the-art production technology, several model series 
can be manufactured flexibly and efficiently according to customer wishes on 
a single assembly line. Precision and quality are guaranteed at all times 
since the plant operates to the high standards of the worldwide production network of the BMW Group. As a centre of expertise for BMW X models, Spartanburg will enlarge its role within this network. In the medium term, annual production will be increased from the current level of 140,000 units 
to 240,000 vehicles. This makes the plant a key compensatory factor 
in relation to currency fluctuations as part of natural hedging.

Robot technology – the basis for precise and efficient processes.

Over 300 robots are used in the manufacture of the body of the BMW X6. 
The welding process in particular is virtually 100 per cent automated. The body of the BMW X6 is made of ultra-high-strength steel in key areas and precision is required in processing this material, which is why robot technology is used 
so extensively here. The high-tech machines apply the bonding material required for maximum strength by means of optical monitoring systems, for example. Weld and bond seams are checked non-destructively using ultrasound devices. In-line laser and measuring cameras are used so as to ensure that the body of this completely new vehicle type conforms to precise measurements. This reduces process times and guarantees that a high 
level of quality is consistently maintained.

At the so-called “wedding”, the engine, transmission and chassis are installed in the BMW X6 on an automated basis. There are ten optical monitoring systems which carry out ongoing quality controls directly during the 
process cycle. These check the installation data collected against pre-defined reference data. 

Robots take care of window pane installation – 
installation time halved.

Window pane assembly in the BMW X6 is carried out at two robot workstations. Bond application and positioning of the panes is performed 
by a camera-controlled, high-precision measuring system. In the first operation, a robot applies the bonding agent onto the edges of the rear window and 
the side windows and mounts the rear window. The second robot applies 
the bonding agent to the windscreen and mounts it onto the body. Only the side panes are then installed by hand. This reduces process time by more 
than half.

Work areas in BMW X6 production have been further improved according to ergonomic criteria. Extensive freedom to manoeuvre vehicles into the best possible working position facilitates the installation of the various components.

BMW Spartanburg plant – a 16-year success story.

The foundation stone for the BMW plant in Spartanburg was laid in 1992, 
with production of the BMW Z3 Roadster starting there three years later. 
To date, the BMW Group has invested over 2.7 billion US dollars in the plant and currently employs a workforce of some 4,500. The first BMW X5 came 
off the Spartanburg assembly line in September 1999 and by June 2005 the plant had already supplied the 500,000th BMW X5. This successful model 
of the SAV segment is now exported to over 120 countries. 

The BMW Spartanburg plant also produces the BMW X6 for the entire 
world market. Every vehicle is manufactured individually according to customer wishes, and all manufacturing processes are subject to the high quality standards of the BMW Group.

Sustainable production: significant reduction of CO2 emissions.

The BMW production plant is also exemplary in its preservation of resources. 
In May 2006 the plant converted the energy supply of its paintshop to methane gas which is extracted from a disposal site several miles away. This saves around 60,000 tons of CO2 a year – equivalent to the annual heating energy needs of about 15,000 American households. At the same time this measure reduces the plant’s annual energy costs by a six-digit euro figure. As a 
result the BMW Spartanburg plant received the “Energy Partner of the Year” award from the US Environmental Protection Agency (EPA) in 2007. 












9.	Production: �Expertise for the X models in a powerful global network.








8.	Equipment and accessories: �Exclusive sportiness and �innovative details.



































